M00 F0317 Program Stop
M01 F0304 Optional Stop
M02 F0305 End of Program
M03 F0300 Spindle forward
M04 F0301 Spindle backward
M05 F0302 Spindle stop
M06 F0303 Auto change tool
M08 F0310 Coolant on
M09 F0311 Coolant off
M10 F0312 A axis Clamp
M11 F0313 A axis Release
M16 F0260 Release tool
M17 F0261 Clamp tool
M18 F0283 Cancel Spindle halt
M19 F0262 Spindle halt
M20 F0325 Spindle no gear instruction
M22 F0264 arm startup 
M26 F0275 Startup Peck drilling
M27 F0276 Stop Peck drilling
M28 F0323 Cancel rigid tapping
M29 F0322 Rigid tapping
M30 F0280 End of Program
M35 F0281 Startup screw peck drilling
M36 F0282 Stop screw peck drilling
M44 F0267 Spindle blow start
M45 F0270 Spindle blow stop
M50 F0271 Auto change tool start
M51 F0272 Auto change tool stop
M53 F0273 Is right tool after change?
M55 F0274 Have tool in spindle?
%
X0000     1st axis positive travel limit
X0001     1st axis negative travel limit
X0002     2nd axis positive travel limit
X0003     2nd axis negative travel limit
X0004     3rd axis positive travel limit
X0005     3rd axis negative travel limit
X0006     4th axis positive travel limit
X0007     4th axis negative travel limit
X0010     1st axis zero return dec
X0011     2nd axis zero return dec
X0012     3rd axis zero return dec
X0013     4th axis zero return dec
X0014     Emergency switch
X0015     External cycle start
X0016     External Pause
X0017     Pressure switch detection
X0020     Low lubricant level
X0021     Undefined
X0022     Cooling motor overheat
X0023     Hydraulic motor overheat
X0024     External tool release/clamp
X0025     Tool release detection
X0026     Tool clamp detection
X0027     Spindle unit alarm
X0030     Edit Lock
X0031     Operate Lock
X0032     Arm braking signal
X0033     Arm with a tool check signal
X0034     Arm zero pos. check signal
X0035     MAG.rotation motor overload
X0036     Arm motor overload
X0037     Coolant motor overload
X0040     Hand unit enable
X0041     1st spindle gear in-pos
X0042     2nd spindle gear in-pos
X0043     3rd spindle gear in-pos
X0044     Check status of spindle
X0045     Undefined
X0046     Spindle speed in-position
X0047     Spindle zero detection
X0050     Spindle orientation in-pos
X0051     POT vertical check
X0052     POT horizon check
X0053     MAG.counter
X0054     
X0055     MAG.zero return in-pos check
X0056     Undefined
X0057     Spindle alarm
X0060     external MPG 1st axis selection
X0061     external MPG 2nd axis selection
X0062     external MPG 3rd axis selection
X0063     external MPG 4th axis selection
X0064     external MPG step 0.001
X0065     external MPG step 0.01
X0066     external MPG step 0.1
X0067     external emergent halt
X0070     Speed/Pos shift finish signal
X0071     Spindle Orentation finish
X0072     Spindle speed arrival
X0073     Spindle speed zero
Y0000     Vertical axis brake hold
Y0001     Cooling
Y0002     Tool release or clamp
Y0003     Program end(M30)and power off
Y0004     Spindle brake
Y0005     Spindle act
Y0006     Red alarm light
Y0007     Yellow alarm light
Y0010     Green alarm light
Y0011     Swarf control
Y0012     Lubricant control
Y0013     Machine illumination
Y0014     Undefined
Y0015     Spindle blow
Y0016     Undefined
Y0017     Undefined
Y0020     Spindle enable
Y0021     Spindle orientation
Y0022     Spindle forward
Y0023     Spindle reverse
Y0024     Hand unit light
Y0025     Arm running
Y0026     Undefined
Y0027     Speed/Pos mode of spindle
Y0030     MAG. rotation forward
Y0031     MAG. rotation backward
Y0032     POT vertical
Y0033     POT horizon 
Y0034     Spindle gear1(freq convert\IO)
Y0035     Spindle gear2(freq convert\IO)
Y0036     Spindle gear3(freq convert\IO)
Y0037     Undefined
Y0040     Undefined
Y0041     Undefined
Y0042     Undefined
Y0043     Undefined
Y0044     Undefined
Y0045     Undefined
Y0046     Undefined
Y0047     Undefined
Y0050     Undefined
Y0051     Undefined
Y0052     Undefined
Y0053     Undefined
Y0054     Undefined
Y0055     Undefined
Y0056     Undefined
Y0057     Undefined
Y0060     Spindle CW
Y0061     Spindle CCW
Y0062     Spindle Enable
Y0063     Spindle Orentation
Y0064     Spindle speed/pos shfit
Y0065     Spindle zero hold
K0060     1st axis limit on-off select(0:2,1:1)
K0061     2nd axis limit on-off select(0:2,1:1)
K0062     3rd axis limit on-off select(0:2,1:1)
K0063     4th axis limit on-off select(0:2,1:1)
K0064     1st axis zero on/off is normal open?
K0065     2nd axis zero on/off is normal open?
K0066     3rd axis zero on/off is normal open?
K0067     4th axis zero on/off is normal open?
K0070     Reserved
K0071     Reserved
K0072     Reserved
K0073     4th axis limit alarm reverse
K0074     Canel 4th axis hard limit(Y/N)
K0075     Reserved
K0076     Reserved
K0077     Use mode of spindle pos(Y/N)
K0080     spindle pos. check is closure
K0081     Release/clamp ctrl by panel
K0082     Not use release/clamp device
K0083     Use auto lubricate equipment
K0084     Spindle has switch device(Y/N)
K0085     spindle speed in pos check is closure
K0086     spindle speed mode is closure(Y/N)
K0087     Mode of spindle switch hasn't check On-off
K0090     hasn't On-off of spindle in-pos(Y/N)
K0091     Lub.press or oil level check valid(Y/N)
K0092     Air pressure check valid(Y/N) 
K0093     A switch for gear check(Y/N)
K0094     If MAG.motor overload check valid
K0095     If Arm motor overload check valid
K0096     If cool motor overload check valid 
K0097     Reserved 
K0100     Reserved 
K0101     MAG. have on-off of return zero
K0102     MAG. on-off of return zero is contact closure
K0103     MAG. on-off of advance is contact closure
K0104     MAG. on-off of restract is contact closure
K0106     Setting of MAG. origin is valid
K0107     MAG. is in debug mode
K0110     Prompt spindle no. on manual release/clamp
K0112     Clean Alarm of No.1244 by modify para.
K0113     Clean alarm info of No.1244
K0114     Reserved
K0115     Reserved
K0116     Reserved
K0117     Reserved
K0120     If arm brake sig.is normal open
K0121     If with Tool sig.is normal open
K0122     If arm zero sig.is normal close 
K0123     If cur.T.head check is normal close
K0124     Reserved
K0125     Reserved
K0126     Reserved
K0127     Arm enters debugging mode(Y/N)
K0134     1st axis unuse origin swtich(Y/N)
K0135     2nd axis unuse origin swtich(Y/N)
K0136     3rd axis unuse origin swtich(Y/N)
K0137     4th axis unuse origin swtich(Y/N)
K0140     是否使用分度工作台夹松装置
K0141     工作台分度是否自动松夹
K0142     工作台夹松是否无检测开关
K0143     分度工作台禁止手动手轮单段
K0144     分度台松开状态是否允许移动XYZ轴
K0145     分度工作台松开夹紧后是否断开输出
K0146     Reserved
K0147     分度工作台进入调试模式
K0500     1st axis forward memory
K0501     2nd axis forward memory
K0502     3rd axis forward memory
K0503     4th axis forward memory
K0505     3rd return to 1st reference end
K0506     3rd return to 2nd reference end
A0000     Abnormal air pressure
A0001     Abnormal lubricant
A0002     Abnormal lubrication motor
A0003     Abnormal cooling motor
A0004     Abnormal chip cleaner motor
A0005     Abnormal pressure oil pump motor
A0006     Abnormal spindle cooling unit
A0007     Abnormal machine light
A0010     Abnormal temp. of MAC ctrl box
A0011     Abnormal temperature of MAC bed
A0012     Abnormal MAC. vibration frequency
A0013     Abnormal pressure oil temp.
A0014     oil pressure low
A0015     machine no ready 
A0016     Cann't rotate as spindle gear abnormal
A0017     Need run T code before M06
A0020     Spindle invalid on tool unstuck
A0021     Can't release tool rotating spindle
A0022     Re-affirm tool no. as tool abnormal stop
A0023     spindle invalid as arm not in origin
A0024     abnormal spindle tool clamping
A0025     abnormal spindle tool releasing
A0026     abnormal spindle unit temperature
A0027     abnormal spindle speed
A0030     abnormal spindle motor enabling
A0031     abnormal spindle orientation in-pos detect
A0032     abnormal spindle gear shifting
A0033     Arm invalid as not in origin 
A0034     POT invalid as in vertial
A0035     Execute MAC.zero before M06 
A0036     Can't change tool on spindle unstuck 
A0037     Can't change tool as POT not in level
A0040     abnormal tool storage rotation in-pos
A0041     MAG.rotation motor overload
A0042     Arm motor overload
A0043     abnormal tool storage move in-pos 
A0044     abnormal tool storage zero return
A0045     need return zero as tool origin lose
A0046     POT vertical in horizon abnormal
A0047     Spindle invalid as POT not in level
A0050     Need return zero as tool abnormal
A0051     POT vertical check abnormal
A0052     POT horizon check abnormal
A0053     setting of tool zero is valid
A0054     Can't change tool as MAG is abnormal 
A0055     Tool no. haven't or repeat in tool table
A0056     Spindle re/cl check abnormal
A0057     Spindle orient sequence abnormal
A0060     T code can't be executed 
A0061     Can't advance as S has tool
A0062     Can't advance as S same cur tool of MAG. 
A0063     Power off please
A0064     Can't move Z on tool clamp
A0065     be careful of operate in MAG. adjust mode
A0066     Can't Startup in MAG. adjust mode
A0067     Can't return origin in tool clamp
A0070     Can't return change pos in tool clamp
A0071     Can't ret change pos as S hasn't orientate
A0072     Can't return change pos as MAG abnormal
A0073     Can't change tool as T number is abnormal
A0074     Can't startup in ret change pos by manual
A0075     Can't restract as it's not in Origin
A0076     Over safety position
A0077     Be careful for arm debug mode 
A0080     Mode of spindle Speed/Pos is abnormal
A0081     Mode of spindle Pos/Speed is abnormal
A0082     Gear shift disabled in spi. running
A0083     Can't start arm as POT not vertical
A0084     Arm disabled as not in origin 
A0085     Arm stop abnormally 
A0086     Arm with a tool check abnormal 
A0087     Arm disabled as S not orient
A0090     Arm disabled as tool clamp  
A0091     Arm disabled as tool unclamp 
A0092     Can't retract as arm not in origin
A0093     Can't retract as arm not in origin
A0094     MAG.invalid as arm not in origin
A0095     MAG.invalid as POT in level 
A0096     Arm invalid as Z not return to 2nd reference 
A0097     Arm origin pos check abnormal
A0100     MAG.stop forcely as normal rotation
A0110     分度工作台松开检测异常
A0111     分度工作台夹紧检测异常
A0112     分度工作台夹紧装置未启用
A0113     分度工作台未松开不可旋转
A0114     分度工作台未夹紧不可移动
A0115     安全门未关上不可循环启动
A0116     分度工作台未夹紧不可启动
A0200     Lub.pressure or oil level low
R0104     MT-刀库回零
R0105     MT-刀库正转
R0106     MT-刀库反转
R0107     MT-刀库倒刀
R0110     MT-刀库回刀
R0111     循环启动信号上升沿
R0300     主轴正转上升沿
R0301     主轴反转上升沿
R0450     主轴速度到达
R0451     主轴位置/速度状态检测
R0452     取消刚性攻丝信号
R0453     T代码辅助功能选通信号上升沿
R0454     主轴位置模式切换完成
R0455     主轴位置模式延时检测
R0456     刚性攻丝指令延时完成
R0457     主轴定向延时完成
R0460     主轴位置模式时定位完成延时
R0462     当前刀盘刀具检测开关
R0463     主轴刀具检测开关
R0464     刀库回零完成
R0470     自动运行时取消刚性攻丝信号
R0471     手动运行时取消刚性攻丝信号
R0472     取消刚性攻丝指令延时完成
R0473     主轴速度模式切换完成
R0474     主轴速度模式延时检测
R0480     主轴位置/速度模式
R0483     主轴定向输入
R0484     使用主轴位置模式
R0490     主轴正转
R0491     主轴反转
R0492     刀库正转/反转到位延迟检测
R0493     刀库旋转中延迟检测
R0495     Z轴返回第一参考点结束标志
R0497     主轴制动延时断开
R0500     主轴模拟量齿轮选择信号
R0501     自动,录入,回零,DNC方式检测
R0502     GR1齿轮选择信号延时检测
R0503     GR2齿轮选择信号延时检测
R0504     GR3齿轮选择信号延时检测
R0505     是否执行T指令
R0510     自动运行信号取反
R0512     刀库前进条件1
R0551     主轴I/O点控制1档信号
R0552     主轴I/O点控制2档信号
R0553     主轴I/O点控制3档信号
R0560     主轴I/O点控制信号输入
R0561     主轴一档延时检测
R0562     主轴二档延时检测
R0563     主轴三档延时检测
R0564     GR1齿轮选择信号(输入)
R0565     GR2齿轮选择信号(输入)
R0566     GR3齿轮选择信号(输入)
R0567     主轴换档是否到位
R0590     逻辑0状态
R0610     刀库使用中禁止模式转换
R0612     自动,录入,DNC方式检测
R0634     主轴定向输入
R0635     主轴定向输入上升沿
R0640     主轴旋转条件
R0641     主轴正转输入
R0642     主轴停止输入
R0643     主轴反转输入
R0644     主轴定向输入
R0645     主轴正转延时完成
R0646     主轴反转延时完成
R0666     主轴空档指令输入
R0667     M5延迟完成
R0670     M代码辅助功能结束信号
R0671     循环启动输入
R0684     非手轮，非单步的方式
R0685     手动,单步方式检测
R0686     手动,单步,手轮方式检测
R0687     回零,手轮方式检测
R0690     手动参考点仅控制1个轴
R0703     MT-手动进给轴 +4th
R0707     MT-手动进给轴 -4th
R0715     手轮方式第1轴轴选自锁
R0716     回零方式第1轴自锁
R0717     手轮方式第2轴轴选自锁
R0720     回零方式第2轴自锁
R0721     手轮方式第3轴轴选自锁
R0722     回零方式第3轴自锁
R0723     手轮方式第4轴轴选自锁
R0724     回零方式第4轴自锁
R0725     超程检测
R0743     主轴换档延时完成
R0744     换档到位信号
R0745     换档到位信号延时断开
R0750     主轴停止输入1
R0760     分度工作台松开
R0761     分度工作台松开完成延时
R0762     分度工作台夹紧完成延时
R0763     分度工作台松开检测延时
R0764     分度工作台夹紧检测延时
R0765     分度工作台松开延时完成
R0766     分度工作台夹紧延时完成
R0767     分度工作台松开完成信号
R0770     分度工作台夹紧完成信号
R0772     分度工作台位置检测
R0781     手动夹/松刀控制
R0782     刀具松紧
R0783     主轴刀具松开完成延时
R0784     主轴刀具夹紧完成延时
R0785     主轴刀具松开检测延时
R0786     主轴刀具夹紧检测延时
R0787     主轴停止
R0801     1秒脉冲
R0802     刀套垂直检测
R0803     刀套水平检测
R0804     刀套水平检测上升沿
R0805     刀库回零到位
R0806     主轴定位延时检测
R0810     主轴正转检测延时
R0811     主轴反转检测延时
R0815     主轴定向完成信号
R0816     上电初始化脉冲
R0817     手动设置刀库原点
R0820     手动设置刀库原点
R0821     松刀检测
R0823     紧刀检测
R0831     刀具表中无指令刀号或指令刀号重复
R0834     循环启动条件
R0846     寻刀中
R0861     刀库计数/到位
R0864     主轴定向完成信号延时检测
R0865     主轴旋转1
R0866     主轴旋转条件不足
R0867     主轴旋转2
R0870     刀库前进条件检测
R0875     第1轴正限位中间继电器
R0876     第2轴正限位中间继电器
R0877     第3轴正限位中间继电器
R0880     第4轴正限位中间继电器
R0881     第1轴负限位中间继电器
R0882     第2轴负限位中间继电器
R0883     第3轴负限位中间继电器
R0884     第4轴负限位中间继电器
R0900     主轴上是否有刀
R0902     主轴与刀库当前的刀号是否相同
R0903     轴选键信号按动有效检测
R0904     回零,单步,手动,手轮方式检测
R0915     手动回换刀位置状态
R0916     刀套水平检测
R0920     主轴定向条件
R0932     紧刀上升沿检测
R0937     松刀上升沿检测
R0940     加工运行中刀库在进刀位置
R0942     刀库是否进入调整模式
R0955     主轴点动输入
R0956     主轴点动输入自锁
R0957     主轴点动延时断开
R0960     主轴点动输入
R0965     T代码辅助功能选通信号下降沿
R0984     刀库旋转中
R0986     刀库自锁一个刀位
R0993     T码刀号是否正常
R0996     主轴刀号清零
R1000     旋转刀库的条件
R1001     手动刀库正转按键延时
R1002     手动刀库反转按键延时
R1003     手动刀库正转输入
R1004     手动刀库反转输入
R1005     刀库旋转到位信号
R1006     刀库手动正转
R1007     刀库手动反转
R1010     刀库正转中
R1012     刀库反转中
R1013     刀库旋转
R1014     刀库旋转并计数
R1015     刀库计数正反转判断
R1016     刀库旋转计数器
R1017     刀库回零按键信号
R1021     刀库回零完毕信号
R1022     刀库回零旋转保持中间继电器
R1023     刀库回零完成
R1024     刀库旋转中
R1025     刀库旋转中延迟检测
R1026     刀库旋转延迟检测
R1030     刀库自动旋转
R1031     刀库正反转判断
R1032     刀库自动正转
R1033     刀库自动反转
R1051     指令刀号为0
R1052     换刀条件
R1053     条件满足产生换刀指令脉冲
R1054     自动换刀开始
R1055     自动机械手动作开始
R1056     还刀时的寻刀开始
R1057     还刀时的寻刀开始
R1060     还刀时的寻刀完成
R1061     抓新刀时的寻刀开始
R1063     指令刀号是否等于主轴刀号
R1064     寻刀结束子程序状态
R1071     刀库前进条件
R1072     刀套垂直方向
R1073     刀套垂直自锁
R1074     刀套水平方向
R1075     刀套水平自锁
R1076     刀套垂直延时检测
R1077     刀套水平延时检测
R1082     刀套垂直完成延时
R1083     刀套水平完成延时
R1091     刀套垂直完成
R1100     主轴空档延时完成
R1200     寻刀中
R1203     已找到所寻刀
R1206     刀库自动寻刀中
R1207     自动进刀信号
R1210     刀套垂直完成
R1211     刀套垂直完成
R1212     主轴刀具松开完成
R1213     刀库自动寻刀结束
R1500     刀具功能选通
R1505     调用1号子程序结束
R1520     当前刀号是否等于指令刀号
R1521     当前刀号是否等于指令刀号
R1526     手动换刀手运行
R1530     指令刀号等于主轴刀号
R1540     自动机械手动作结束
R1541     复位C50
R1547     z轴返回第一参考点结束保持
R1550     机械手动作开始
R1551     机械手回原点位置下降沿
R1552     自动紧刀信号
R1553     机械手持刀下降沿
R1556     机械手动作开始下降沿
R1557     自动松刀信号
R1570     机械手持刀
R1571     机械手下降旋转180度上升
R1572     机械手回原点位置
R1573     自动机械手动作开始上升沿
R1574     机械手回原点位置上升沿
R1583     手动换刀手运行
R1584     手动换刀手运行条件
R1800     机械手刹车信号
R1801     机械手持刀检测信号
R1802     机械手零位检测信号
R1803     机械手刹车信号下降沿
R1804     机械手刹车信号上升沿
R1806     MT-换刀手
R1807     MT-换刀手上升沿
R1811     机械手持刀检测信号上升沿
R1812     机械手零位检测信号上升沿
R5100     梯形图第一次扫描接通
R5110     一直关断
R5116     1s周期信号
T0001     主轴正转完成延时器
T0002     主轴反转完成延时器
T0003     主轴换档完成延时器
T0004     主轴定位完成延时器
T0005     辅助功能完成延时器
T0006     主轴换档延时器
T0007     主轴刀具松开完成延时器
T0008     主轴刀具夹紧完成延时器
T0009     主轴刀具松开到位检测时间
T0010     主轴刀具夹紧到位检测时间
T0011     M代码辅助功能延时完成
T0012     T代码辅助功能延时完成
T0013     主轴定位检测时间
T0014     主轴正转检测时间
T0015     主轴反转检测时间
T0016     润滑关时间(单位:分钟)
T0017     润滑开时间(单位:秒)
T0018     主轴定位延时检测时间设置
T0019     主轴点动延时器
T0020     程序再启动延时器
T0021     主轴一档延时检测时间
T0022     主轴二档延时检测时间
T0023     主轴三档延时检测时间
T0024     主轴速度位置模式转换检测时间
T0025     M29执行完成时间(无检测信号时有效)
T0026     无检测信号时,主轴位置模式定位完成时间
T0027     M28执行完成时间(无检测信号时有效)
T0028     主轴位置速度模式转换检测时间
T0029     主轴制动时间
T0030     主轴档位1无检测开关时换档延迟时间
T0031     主轴档位2无检测开关时换档延迟时间
T0032     主轴档位3无检测开关时换档延迟时间
T0033     主轴档位控制无检测开关时档位取消延迟完成
T0034     M5完成延迟时间
T0035     主轴换档完成延时断开
T0036     分度工作台松开完成延时
T0037     分度工作台夹紧完成延时
T0038     分度工作台松开检测延时
T0039     分度工作台夹紧检测延时
T0100     刀库手动旋转延迟时间1
T0101     刀库手动旋转延迟时间2
T0102     刀库停止延迟检测时间设置
T0103     刀库旋转延迟检测时间设置1
T0104     刀套垂直延迟检测时间设置
T0105     刀套水平延迟检测时间设置
T0106     刀套垂直完成延时器
T0107     刀套水平完成延时器
T0108     刀库旋转延迟检测时间设置 2
T0109     刀库旋转异常强制停止时间设置
T0110     机械手持刀及回原位延时检测
T0111     机械手下降交换刀具延时检测
D0000     主轴刀号显示
D0001     1号刀具号
D0002     2号刀具号
D0003     3号刀具号
D0004     4号刀具号
D0005     5号刀具号
D0006     6号刀具号
D0007     7号刀具号
D0008     8号刀具号
D0009     9号刀具号
D0010     10号刀具号
D0011     11号刀具号
D0012     12号刀具号
D0013     13号刀具号
D0014     14号刀具号
D0015     15号刀具号
D0016     16号刀具号
D0017     17号刀具号
D0018     18号刀具号
D0019     19号刀具号
D0020     20号刀具号
D0021     21号刀具号
D0022     22号刀具号
D0023     23号刀具号
D0024     24号刀具号
D0100     刀库容量
D0241     T码刀号
D0243     当前刀库刀套号
D0245     主轴刀具号
end //    Symbol of end 
