PLC VER1.0
PLC_ORGANIZATION
TOTALSTEPS	2584
0000    END1
0001    LD      X0024.0
0002    AND     K0010.0
0003    OUT     G0008.6
0004    LD      F0003.3
0005    OR      F0003.4
0006    OR      F0003.5
0007    OUT     R0335.0
0008    LD      F0003.5
0009    OR      F0003.4
0010    OR      F0003.3
0011    LD      F0003.2
0012    AND     G0019.7
0013    ORB
0014    OR      F0004.5
0015    OUT     R0335.7
0016    LDI     R0335.0
0017    OUT     R0335.1
0018    LD      R0335.0
0019    OR      F0003.6
0020    OUT     R0017.0
0021    LD      F0003.0
0022    OR      F0003.1
0023    OUT     R0138.0
0024    LD      R0138.0
0025    OR      F0003.2
0026    OUT     R0138.1
0027    LDI     R0111.0
0028    MOVN    0001 K0009 G0043
0029    MOVN    0001 K0004 G0030
0030    MOVN    0001 K0001 G0010
0031    MOVN    0001 K0005 G0012
0032    LDI     R0111.0
0033    RST     K0002.3
0034    RST     K0002.4
0035    RST     K0006.3
0036    RST     K0006.7
0037    RST     K0007.6
0038    MOVN    0001 D0410 G0201
0039    MOVN    0001 31 G0130
0040    LD      X0018.0
0041    OR      X0018.1
0042    OR      X0018.2
0043    OR      X0018.3
0044    OR      X0018.4
0045    OR      X0018.5
0046    OR      X0019.3
0047    OUT     R0135.4
0048    DIFU    R0135.5
0049    LD      X0019.3
0050    AND     G0043.0
0051    ANI     G0043.1
0052    ANI     G0043.2
0053    ALT     G0043.5
0054    LD      R0135.5
0055    CALL    P0019
0056    MOVN    0001 G0043 K0009
0057    LD      F0003.0
0058    OR      F0003.1
0059    OUT     Y0023.3
0060    LD      F0003.2
0061    OUT     Y0023.2
0062    LD      F0003.3
0063    OUT     Y0023.5
0064    LD      F0003.5
0065    OUT     Y0023.6
0066    LD      F0003.6
0067    OUT     Y0023.7
0068    LD      F0004.5
0069    OUT     Y0023.4
0070    LD      F0003.4
0071    OUT     Y0018.2
0072    LD      R0100.0
0073    ORI     R0100.0
0074    OUT     G0008.4
0075    OUT     R0111.0
0076    LD      K0015.7
0077    CALL    P0050
0078    LDI     K0015.7
0079    MOVN    0001 31 G0114
0080    MOVN    0001 31 G0116
0081    LD      X0002.7
0082    ANI     K0015.6
0083    LDI     X0002.7
0084    AND     K0015.6
0085    ORB
0086    ANI     K0015.7
0087    OUT     A0010.0
0088    LDI     X0000.5
0089    ANI     F0210.3
0090    OUT     R0008.4
0091    LDI     R0008.4
0092    ORI     F0211.4
0093    ANI     F0035.0
0094    OUT     G0029.6
0095    LD      F0001.1
0096    ANI     K0010.1
0097    OR      R0008.4
0098    OUT     R0270.0
0099    LD      X0001.4
0100    ANI     F0210.6
0101    OUT     R0270.1
0102    LDI     X0000.1
0103    ANI     F0210.5
0104    OUT     R0270.2
0105    LD      F0009.7
0106    LD      F0009.6
0107    AND     R0000.0
0108    ORB
0109    OUT     R0270.4
0110    LD      F0197.1
0111    AND     K0010.2
0112    AND     F0003.3
0113    OUT     R0270.3
0114    LD      X0023.0
0115    OR      R0270.1
0116    OR      R0270.3
0117    OUT     R0602.0
0118    LD      R0602.0
0119    AND     G0008.5
0120    OUT     G0007.2
0121    LDI     X0022.7
0122    ANI     R0270.2
0123    ANI     R0270.4
0124    OUT     G0008.5
0125    LD      F0000.4
0126    OUT     Y0021.0
0127    LD      F0000.5
0128    OUT     Y0020.0
0129    LD      R0111.0
0130    CALL    P0010
0131    LD      R0111.0
0132    CALL    P0011
0133    LD      R0111.0
0134    CALL    P0012
0135    LD      F0127.3
0136    CALL    P0013
0137    LD      F0127.4
0138    CALL    P0014
0139    LD      F0094.0
0140    OR      F0096.0
0141    OR      F0098.0
0142    OR      F0100.0
0143    OUT     Y0022.7
0144    LD      F0094.1
0145    OR      F0096.1
0146    OR      F0098.1
0147    OR      F0100.1
0148    OUT     Y0022.6
0149    LD      F0094.2
0150    OR      F0096.2
0151    OR      F0098.2
0152    OR      F0100.2
0153    OUT     Y0022.5
0154    LD      F0094.3
0155    OR      F0096.3
0156    OR      F0098.3
0157    OR      F0100.3
0158    AND     F0127.3
0159    OUT     Y0022.4
0160    LD      F0094.4
0161    OR      F0096.4
0162    OR      F0098.4
0163    OR      F0100.4
0164    AND     F0127.4
0165    OUT     Y0021.2
0166    LDI     F0001.1
0167    ANI     F0001.0
0168    OUT     R0466.3
0169    LD      R0016.0
0170    LD      R0015.0
0171    AND     F0205.2
0172    ORB
0173    AND     F0004.5
0174    AND     R0466.3
0175    ANI     Y0022.7
0176    AND     G0130.0
0177    OUT     R0015.0
0178    LD      R0016.1
0179    LD      R0015.1
0180    AND     F0205.2
0181    ORB
0182    AND     F0004.5
0183    AND     R0466.3
0184    ANI     Y0022.7
0185    AND     G0130.0
0186    OUT     R0015.1
0187    LD      R0016.4
0188    LD      R0015.4
0189    AND     F0205.2
0190    ORB
0191    AND     F0004.5
0192    AND     R0466.3
0193    ANI     Y0022.6
0194    AND     G0130.1
0195    OUT     R0015.4
0196    LD      R0016.5
0197    LD      R0015.5
0198    AND     F0205.2
0199    ORB
0200    AND     F0004.5
0201    AND     R0466.3
0202    ANI     Y0022.6
0203    AND     G0130.1
0204    OUT     R0015.5
0205    LD      R0016.2
0206    LD      R0015.2
0207    AND     F0205.2
0208    ORB
0209    AND     F0004.5
0210    AND     R0466.3
0211    ANI     Y0022.5
0212    AND     G0130.2
0213    OUT     R0015.2
0214    LD      R0016.3
0215    LD      R0015.3
0216    AND     F0205.2
0217    ORB
0218    AND     F0004.5
0219    AND     R0466.3
0220    ANI     Y0022.5
0221    AND     G0130.2
0222    OUT     R0015.3
0223    LD      R0016.0
0224    OR      R0015.0
0225    AND     F0000.6
0226    AND     G0130.0
0227    OUT     G0100.0
0228    LD      R0016.1
0229    OR      R0015.1
0230    AND     F0000.6
0231    AND     G0130.0
0232    OUT     G0102.0
0233    LD      R0016.4
0234    OR      R0015.4
0235    AND     F0000.6
0236    AND     G0130.1
0237    OUT     G0100.1
0238    LD      R0016.5
0239    OR      R0015.5
0240    AND     F0000.6
0241    AND     G0130.1
0242    OUT     G0102.1
0243    LD      R0016.2
0244    OR      R0015.2
0245    AND     F0000.6
0246    AND     G0130.2
0247    OUT     G0100.2
0248    LD      R0016.3
0249    OR      R0015.3
0250    AND     F0000.6
0251    AND     G0130.2
0252    OUT     G0102.2
0253    LD      F0127.3
0254    CALL    P0020
0255    LD      F0127.4
0256    CALL    P0021
0257    LD      R0017.0
0258    CALL    P0008
0259    LDI     R0017.0
0260    CALL    P0009
0261    LD      F0007.0
0262    DECB    0004 F0010 8 R0004
0263    DECB    0004 F0010 29 R0005
0264    DECB    0004 F0010 14 R0022
0265    LD      R0004.1
0266    AND     F0001.3
0267    OUT     R0119.0
0268    LD      R0004.3
0269    AND     F0001.3
0270    OUT     R0119.1
0271    LD      X0021.4
0272    LD      R0004.0
0273    ANI     R0013.0
0274    ORB
0275    LD      R0119.0
0276    OR      F0009.4
0277    LD      R0270.0
0278    ANI     F0001.0
0279    ORB
0280    AND     R0013.0
0281    ORB
0282    ALT     R0013.0
0283    LD      R0013.0
0284    OUT     Y0000.0
0285    OUT     Y0023.0
0286    LD      R0004.2
0287    ANI     R0013.1
0288    LD      R0119.1
0289    OR      F0009.4
0290    OR      R0270.0
0291    AND     R0013.1
0292    ORB
0293    ALT     R0013.1
0294    LD      R0013.1
0295    OUT     Y0002.7
0296    LD      F0007.0
0297    DECB    0004 F0010 32 R0032
0298    LD      R0032.1
0299    AND     F0001.3
0300    OUT     R0119.2
0301    LD      R0111.0
0302    CMP     0004 0 DT0018 R0469.0
0303    CMP     0004 0 DT0017 R0808.0
0304    LD      R0469.1
0305    AND     R0808.1
0306    CALL    P0016
0307    LDI     R0469.1
0308    AND     R0808.1
0309    CALL    P0017
0310    LD      R0808.2
0311    CALL    P0018
0312    LD      Y0000.1
0313    OUT     Y0020.7
0314    LD      R0022.5
0315    OR      X0025.7
0316    OR      R0008.0
0317    ANI     X0005.2
0318    ANI     F0001.1
0319    ANI     A0000.4
0320    SET     Y0003.0
0321    SET     Y0021.3
0322    OUT     R0008.0
0323    TMRB    T0015 DT0014 R0008.1
0324    LD      R0008.1
0325    OR      A0000.4
0326    ANI     F0001.1
0327    OUT     A0000.4
0328    LD      R0111.0
0329    CALL    P0006
0330    LD      F0007.0
0331    DECB    0004 F0010 0 R0133
0332    LD      R0133.5
0333    AND     F0001.3
0334    OUT     R0143.5
0335    LD      R0133.3
0336    AND     Y0000.3
0337    LD      R0133.4
0338    AND     Y0000.4
0339    ORB
0340    OUT     A0000.3
0341    LD      X0021.5
0342    ANI     R0017.0
0343    OUT     R0017.5
0344    LD      X0021.3
0345    ANI     R0017.0
0346    OUT     R0017.3
0347    LD      X0021.7
0348    ANI     R0017.0
0349    OUT     R0017.4
0350    LD      X0025.5
0351    LDI     R0017.0
0352    OR      K0010.4
0353    ANB
0354    OUT     R0017.2
0355    LDI     R0017.5
0356    ANI     R0143.5
0357    ANI     R0270.0
0358    ANI     F0009.4
0359    ANI     F0035.0
0360    OUT     R0511.0
0361    LD      R0017.4
0362    OR      R0133.3
0363    OR      R0603.0
0364    ANI     Y0000.3
0365    AND     R0511.0
0366    ANI     R0307.6
0367    ANI     R0006.0
0368    ANI     R0008.0
0369    OUT     R0603.0
0370    LD      R0017.2
0371    ANI     Y0000.3
0372    AND     R0511.0
0373    ANI     R0307.6
0374    ANI     R0603.0
0375    ANI     R0008.0
0376    OUT     R0603.1
0377    OUT     Y0021.1
0378    LD      R0603.0
0379    OR      R0603.1
0380    OUT     Y0000.4
0381    OUT     Y0005.3
0382    OUT     G0074.4
0383    LD      F0065.0
0384    OR      R0603.0
0385    OR      R0603.1
0386    OUT     Y0019.1
0387    LD      R0017.3
0388    OR      R0133.4
0389    OR      R0604.0
0390    ANI     Y0000.4
0391    AND     R0511.0
0392    ANI     R0307.6
0393    ANI     R0006.0
0394    ANI     R0008.0
0395    OUT     R0604.0
0396    LD      R0604.0
0397    OUT     Y0000.3
0398    OUT     Y0005.2
0399    OUT     G0074.5
0400    LD      F0065.1
0401    OR      R0604.0
0402    OUT     Y0023.1
0403    LDI     Y0019.1
0404    ANI     Y0023.1
0405    OUT     Y0000.5
0406    OUT     Y0018.0
0407    LD      A0000.4
0408    OR      Y0000.3
0409    OR      Y0000.4
0410    OR      X0024.0
0411    RST     Y0003.0
0412    RST     Y0021.3
0413    LD      Y0000.3
0414    OR      Y0000.4
0415    OUT     R0307.0
0416    LD      R0307.0
0417    SET     R0307.7
0418    LD      R0307.7
0419    CALL    P0015
0420    LD      K0012.6
0421    AND     F0200.4
0422    CALL    P0022
0423    LD      K0012.7
0424    AND     F0200.4
0425    CALL    P0024
0426    LDI     R0001.0
0427    AND     F0003.3
0428    ANI     Y0001.6
0429    ANI     F0000.5
0430    ANI     Y0001.7
0431    AND     K0011.7
0432    OUT     R0076.2
0433    LD      R0076.2
0434    MOVN    0001 D0409 C0023
0435    MOVN    0001 D0409 C0022
0436    LD      K0011.7
0437    ANI     K0011.6
0438    LDI     K0011.7
0439    AND     K0011.6
0440    ORB
0441    MOVN    0001 F0207 DC0001
0442    LD      K0011.7
0443    ANI     K0011.6
0444    CALL    P0030
0445    OUT     G0176.7
0446    LDI     K0011.7
0447    AND     K0011.6
0448    CALL    P0040
0449    LD      K0011.5
0450    CALL    P0026
0451    LD      R0060.3
0452    OR      R0060.4
0453    ANI     R0037.6
0454    ANI     A0000.7
0455    OR      R0185.0
0456    OR      R0046.7
0457    OUT     R0185.2
0458    LD      R0004.0
0459    OR      R0119.0
0460    LD      R0133.3
0461    OR      R0133.4
0462    ANI     R0307.6
0463    ANI     A0000.3
0464    ORB
0465    OR      R0143.5
0466    OR      R0032.0
0467    OR      R0119.2
0468    LD      R0022.5
0469    AND     X0005.2
0470    ORB
0471    OR      R0004.2
0472    OR      R0119.1
0473    LD      R0005.0
0474    AND     X0005.0
0475    ORB
0476    OR      R0006.7
0477    OR      R0007.7
0478    OR      R0185.2
0479    TMRB    T0002 DT0021 R0221.1
0480    LD      F0009.4
0481    OR      F0009.5
0482    OR      F0009.6
0483    OR      F0009.7
0484    TMRB    T0003 160 R0221.2
0485    LD      R0221.1
0486    OR      R0221.2
0487    OR      R0221.3
0488    OR      R0020.7
0489    OR      R0073.7
0490    AND     F0007.0
0491    OUT     R0222.0
0492    LDI     F0007.0
0493    OR      R0222.0
0494    LDI     F0007.2
0495    OR      R0233.0
0496    ANB
0497    LDI     F0007.3
0498    OR      R0211.0
0499    OR      R0211.3
0500    ANB
0501    LD      F0007.0
0502    OR      F0007.2
0503    OR      F0007.3
0504    ANB
0505    OUT     G0004.3
0506    LDI     F0200.4
0507    CALL    P0007
0508    LD      K0010.3
0509    OUT     G0006.4
0510    LD      R0111.0
0511    OUT     G0046.3
0512    LD      F0007.0
0513    CMP     0004 F0010 11 R0099.0
0514    LD      R0050.4
0515    OR      R0050.5
0516    OR      R0060.5
0517    OR      R0060.6
0518    OR      R0061.0
0519    OR      R0061.1
0520    OR      R0061.2
0521    OR      R0046.3
0522    OR      R0060.0
0523    OR      R0060.1
0524    OUT     R0061.7
0525    LD      R0032.0
0526    OR      R0032.1
0527    OR      F0009.4
0528    OR      R0004.6
0529    OR      R0004.7
0530    OR      R0061.7
0531    OR      R0096.0
0532    AND     F0007.0
0533    OUT     R0099.7
0534    LD      R0099.0
0535    OR      R0133.6
0536    OR      R0133.7
0537    ANI     R0099.7
0538    AND     F0007.0
0539    ANI     F0001.1
0540    ANI     R0005.0
0541    ANI     R0022.5
0542    OUT     A0000.0
0543    LD      R0111.0
0544    CALL    P0000
0545    LD      F0003.0
0546    DIFD    R0000.7
0547    LD      F0003.1
0548    DIFD    R0000.6
0549    LD      F0003.0
0550    OR      F0003.1
0551    OR      R0000.6
0552    OR      R0000.7
0553    CALL    P0001
0554    LD      F0003.3
0555    OR      F0003.5
0556    OR      F0003.4
0557    OR      F0003.2
0558    OR      F0004.5
0559    CALL    P0002
0560    LD      F0003.6
0561    RST     Y0019.5
0562    RST     Y0019.6
0563    RST     Y0019.7
0564    RST     Y0021.5
0565    LD      F0200.4
0566    CALL    P0003
0567    LDI     F0200.4
0568    RST     Y0020.6
0569    RST     Y0020.3
0570    LD      R0111.0
0571    CALL    P0004
0572    LD      R0111.0
0573    CALL    P0005
0574    END2
0575    SP      P0000
0576    LD      F0001.7
0577    ANI     F0000.5
0578    OUT     Y0002.2
0579    LD      F0000.5
0580    OUT     Y0002.3
0581    LD      F0001.0
0582    OUT     Y0002.4
0583    SPE
0584    SP      P0001
0585    LD      X0019.4
0586    LD      X0006.3
0587    ANI     R0700.2
0588    AND     R0700.3
0589    ORB
0590    AND     R0138.0
0591    RST     K0006.4
0592    RST     K0006.5
0593    LD      X0019.5
0594    LD      X0006.4
0595    ANI     R0700.2
0596    AND     R0700.3
0597    ORB
0598    AND     R0138.0
0599    SET     K0006.4
0600    RST     K0006.5
0601    LD      X0019.6
0602    LD      X0006.5
0603    ANI     R0700.2
0604    AND     R0700.3
0605    ORB
0606    AND     R0138.0
0607    RST     K0006.4
0608    SET     K0006.5
0609    LD      X0019.7
0610    AND     R0138.0
0611    ANI     K0013.7
0612    SET     K0006.4
0613    SET     K0006.5
0614    LD      K0006.4
0615    AND     K0006.5
0616    AND     K0013.7
0617    AND     R0138.0
0618    RST     K0006.4
0619    SET     K0006.5
0620    LD      X0019.4
0621    OR      X0019.5
0622    OR      X0019.6
0623    OR      X0019.7
0624    OR      R0700.2
0625    AND     R0700.3
0626    OUT     R0700.2
0627    LD      X0006.3
0628    OR      X0006.4
0629    OR      X0006.5
0630    OUT     R0700.3
0631    LD      K0006.4
0632    OUT     G0019.4
0633    LD      K0006.5
0634    OUT     G0019.5
0635    LDI     K0006.4
0636    ANI     K0006.5
0637    AND     R0138.0
0638    OUT     Y0019.7
0639    LD      K0006.4
0640    ANI     K0006.5
0641    AND     R0138.0
0642    OUT     Y0019.6
0643    LDI     K0006.4
0644    AND     K0006.5
0645    AND     R0138.0
0646    OUT     Y0019.5
0647    LD      K0006.4
0648    AND     K0006.5
0649    AND     R0138.0
0650    OUT     Y0021.5
0651    LD      X0021.0
0652    LD      X0006.1
0653    ANI     R0700.0
0654    AND     R0700.1
0655    ORB
0656    AND     F0003.1
0657    RST     K0002.0
0658    SET     K0002.1
0659    RST     K0002.2
0660    LD      X0020.3
0661    LD      X0006.2
0662    ANI     R0700.0
0663    AND     R0700.1
0664    ORB
0665    AND     F0003.1
0666    SET     K0002.0
0667    SET     K0002.1
0668    RST     K0002.2
0669    LD      X0020.5
0670    LD      X0006.0
0671    ANI     R0700.0
0672    AND     R0700.1
0673    ORB
0674    AND     F0003.1
0675    SET     K0002.0
0676    RST     K0002.1
0677    RST     K0002.2
0678    LD      X0020.2
0679    AND     F0003.1
0680    AND     F0127.3
0681    RST     K0002.0
0682    RST     K0002.1
0683    SET     K0002.2
0684    LD      X0020.1
0685    AND     F0003.1
0686    AND     F0127.4
0687    SET     K0002.0
0688    RST     K0002.1
0689    SET     K0002.2
0690    LD      X0020.3
0691    OR      X0020.2
0692    OR      X0020.5
0693    OR      X0021.0
0694    OR      X0020.1
0695    OR      R0700.0
0696    AND     R0700.1
0697    OUT     R0700.0
0698    LD      X0006.0
0699    OR      X0006.1
0700    OR      X0006.2
0701    OUT     R0700.1
0702    LD      K0002.0
0703    OUT     G0018.0
0704    LD      K0002.1
0705    OUT     G0018.1
0706    LD      K0002.2
0707    OUT     G0018.2
0708    LD      G0018.0
0709    ANI     G0018.1
0710    ANI     G0018.2
0711    AND     F0003.1
0712    OUT     Y0019.2
0713    LDI     G0018.0
0714    AND     G0018.1
0715    ANI     G0018.2
0716    AND     F0003.1
0717    OUT     Y0021.4
0718    LD      G0018.0
0719    AND     G0018.1
0720    ANI     G0018.2
0721    AND     F0003.1
0722    OUT     Y0019.4
0723    LDI     G0018.0
0724    ANI     G0018.1
0725    AND     G0018.2
0726    AND     F0003.1
0727    AND     F0127.3
0728    OUT     Y0019.3
0729    LD      G0018.0
0730    ANI     G0018.1
0731    AND     G0018.2
0732    AND     F0003.1
0733    AND     F0127.4
0734    OUT     Y0021.6
0735    SPE
0736    SP      P0002
0737    LD      R0111.0
0738    MOVN    0001 C0001 R0234
0739    CODB    0001 0002 R0234 K0000 , 0 2 1 3
0740    LD      K0000.0
0741    OUT     G0014.0
0742    LD      K0000.1
0743    OUT     G0014.1
0744    LD      K0000.0
0745    AND     K0000.1
0746    OUT     Y0020.2
0747    LD      K0000.0
0748    AND     K0000.1
0749    AND     R0335.7
0750    OUT     Y0019.7
0751    LDI     K0000.0
0752    AND     K0000.1
0753    AND     R0335.7
0754    OUT     Y0019.5
0755    LD      K0000.0
0756    ANI     K0000.1
0757    AND     R0335.7
0758    OUT     Y0019.6
0759    LDI     K0000.0
0760    ANI     K0000.1
0761    OUT     Y0020.5
0762    LDI     K0000.0
0763    ANI     K0000.1
0764    AND     R0335.7
0765    OUT     Y0021.5
0766    LD      F0003.0
0767    OR      F0003.1
0768    OR      F0003.6
0769    OUT     R0010.0
0770    LDI     K0000.0
0771    ANI     K0000.1
0772    OUT     R0003.0
0773    LD      K0000.0
0774    AND     K0000.1
0775    OUT     R0003.1
0776    LD      X0022.5
0777    ANI     R0010.0
0778    ANI     R0003.1
0779    OUT     R0010.1
0780    LD      X0022.2
0781    ANI     R0010.0
0782    ANI     R0003.0
0783    OUT     R0010.2
0784    LD      R0010.1
0785    ANI     R0010.2
0786    CTRC    0000 R0088.7 C0001 3 R0088.0
0787    MOVN    0004 C0001 C0002
0788    LD      R0010.2
0789    ANI     R0010.1
0790    CTRC    0001 R0088.7 C0002 0 R0088.1
0791    MOVN    0004 C0002 C0001
0792    LD      X0019.4
0793    AND     R0335.7
0794    OUT     R0010.7
0795    LD      X0019.6
0796    AND     R0335.7
0797    OUT     R0010.6
0798    LD      X0019.7
0799    AND     R0335.7
0800    OUT     R0010.5
0801    LD      X0019.5
0802    AND     R0335.7
0803    OUT     R0010.4
0804    LD      R0010.7
0805    MOVN    0001 3 C0001
0806    LD      R0010.6
0807    MOVN    0001 1 C0001
0808    LD      R0010.5
0809    MOVN    0001 0 C0001
0810    LD      R0010.4
0811    MOVN    0001 2 C0001
0812    LD      R0010.7
0813    OR      R0010.6
0814    OR      R0010.5
0815    OR      R0010.4
0816    MOVN    0001 C0001 C0002
0817    SPE
0818    SP      P0003
0819    LD      X0022.1
0820    ANI     K0007.1
0821    ANI     X0022.4
0822    AND     F0200.4
0823    ANI     F0002.3
0824    OUT     R0089.0
0825    LD      R0089.0
0826    CTRC    0000 R0075.0 C0006 7 R0075.1
0827    MOVN    0004 C0006 C0007
0828    LD      X0022.4
0829    ANI     K0007.4
0830    ANI     X0022.1
0831    AND     F0200.4
0832    ANI     F0002.3
0833    OUT     R0089.1
0834    LD      R0089.1
0835    CTRC    0001 R0075.7 C0007 0 R0075.6
0836    MOVN    0004 C0007 C0006
0837    LD      X0022.4
0838    OR      X0022.1
0839    MOVN    0001 C0006 R0230
0840    CODB    0001 0003 R0230 G0030 , 7 6 2 3 1 0 4 5
0841    MOVN    0001 G0030 K0004
0842    LD      R0111.0
0843    CMP     0004 7 C0006 K0007.0
0844    CMP     0004 0 C0007 K0007.3
0845    LD      K0007.1
0846    OUT     Y0020.6
0847    LD      K0007.4
0848    OUT     Y0020.3
0849    SPE
0850    SP      P0004
0851    LD      X0019.1
0852    ANI     R0335.1
0853    ALT     K0002.3
0854    LD      K0002.3
0855    ANI     R0335.1
0856    OUT     G0005.6
0857    LD      F0004.4
0858    ANI     R0335.1
0859    OUT     Y0018.4
0860    LD      X0019.0
0861    ANI     F0000.5
0862    ALT     K0002.4
0863    LD      K0002.4
0864    OUT     G0044.1
0865    LD      F0004.1
0866    OUT     Y0018.5
0867    LD      X0019.2
0868    ANI     F0000.5
0869    ANI     R0335.1
0870    ALT     K0006.3
0871    LD      K0006.3
0872    ANI     R0335.1
0873    OUT     G0046.7
0874    LD      F0002.7
0875    ANI     R0335.1
0876    OUT     Y0018.3
0877    LD      X0018.6
0878    ANI     R0335.1
0879    ALT     K0006.7
0880    LD      K0006.7
0881    ANI     R0335.1
0882    OUT     G0046.1
0883    LD      F0004.3
0884    ANI     R0335.1
0885    OUT     Y0018.7
0886    LD      X0018.7
0887    ANI     R0335.1
0888    ALT     K0007.6
0889    LD      K0007.6
0890    ANI     R0335.1
0891    OUT     G0044.0
0892    LD      F0004.0
0893    ANI     R0335.1
0894    OUT     Y0018.6
0895    LD      X0020.0
0896    ANI     R0335.1
0897    ALT     R0000.0
0898    LD      R0000.0
0899    ANI     R0335.1
0900    OUT     Y0021.7
0901    SPE
0902    SP      P0005
0903    LD      F0003.2
0904    AND     X0020.6
0905    LD      R0335.0
0906    OR      F0003.1
0907    OR      F0003.6
0908    OR      F0004.5
0909    OR      F0003.0
0910    AND     R0136.0
0911    ORB
0912    ALT     R0136.0
0913    LD      R0136.0
0914    OUT     G0019.7
0915    OUT     Y0018.1
0916    SPE
0917    SP      P0006
0918    LD      R0005.0
0919    OR      R0004.6
0920    OR      R0004.7
0921    OUT     R0006.0
0922    LD      R0004.6
0923    SET     R0006.6
0924    LD      R0004.7
0925    RST     R0006.6
0926    LD      F0076.3
0927    ANI     A0000.2
0928    LD      R0006.6
0929    ANI     A0000.5
0930    ORB
0931    OUT     Y0005.0
0932    LD      R0005.0
0933    TMRB    T0010 DT0015 A0000.2
0934    LD      R0004.6
0935    TMRB    T0016 DT0029 A0000.5
0936    LD      X0005.0
0937    AND     F0076.3
0938    OUT     G0061.0
0939    OUT     Y0005.1
0940    LD      X0005.0
0941    AND     R0004.6
0942    AND     R0006.6
0943    SET     G0027.7
0944    OUT     R0006.7
0945    LDI     X0005.0
0946    AND     R0004.7
0947    ANI     R0006.6
0948    RST     G0027.7
0949    OUT     R0007.7
0950    SPE
0951    SP      P0007
0952    LD      F0007.2
0953    DECB    0004 F0022 0 R0204
0954    TMRB    T0009 DT0024 R0582.0
0955    LD      R0582.0
0956    TMRB    T0000 DT0019 R0233.0
0957    LDI     R0582.0
0958    LD      R0204.1
0959    ANI     R0205.0
0960    LD      R0204.2
0961    ANI     R0205.1
0962    ORB
0963    LD      R0204.3
0964    ANI     R0205.2
0965    ORB
0966    LD      R0204.4
0967    ANI     R0205.3
0968    ORB
0969    ANB
0970    LD      R0008.4
0971    AND     F0211.4
0972    ORB
0973    OR      R0204.0
0974    MOVN    0001 0 R0205
0975    LD      R0204.1
0976    AND     R0582.0
0977    MOVN    0001 1 R0205
0978    LD      R0204.2
0979    AND     R0582.0
0980    MOVN    0001 2 R0205
0981    LD      R0204.3
0982    AND     R0582.0
0983    MOVN    0001 4 R0205
0984    LD      R0204.4
0985    AND     R0582.0
0986    MOVN    0001 8 R0205
0987    LD      R0205.0
0988    OUT     Y0001.0
0989    LD      R0205.1
0990    OUT     Y0001.1
0991    LD      R0205.2
0992    OUT     Y0001.2
0993    LD      R0205.3
0994    OUT     Y0001.3
0995    SPE
0996    SP      P0008
0997    LD      R0111.0
0998    MOVN    0001 K0005 G0012
0999    LD      X0022.6
1000    ANI     K0006.1
1001    ANI     X0022.3
1002    CTRC    0000 R0770.0 C0004 15 R0770.1
1003    MOVN    0004 C0004 C0005
1004    LD      X0022.3
1005    ANI     K0002.6
1006    ANI     X0022.6
1007    CTRC    0001 R0770.3 C0005 0 R0770.2
1008    MOVN    0004 C0005 C0004
1009    LD      X0022.3
1010    OR      X0022.6
1011    MOVN    0001 C0004 K0005
1012    LD      R0111.0
1013    CMP     0004 15 C0004 K0006.0
1014    CMP     0004 0 C0005 K0002.5
1015    LD      K0002.6
1016    OUT     Y0020.4
1017    LD      K0006.1
1018    OUT     Y0020.1
1019    SPE
1020    SP      P0009
1021    LD      R0111.0
1022    MOVN    0001 K0001 G0012
1023    LD      X0022.6
1024    ANI     K0008.1
1025    ANI     X0022.3
1026    CTRC    0000 R0770.0 C0009 15 R0770.1
1027    MOVN    0004 C0009 C0010
1028    LD      X0022.3
1029    ANI     K0008.4
1030    ANI     X0022.6
1031    CTRC    0001 R0770.3 C0010 0 R0770.2
1032    MOVN    0004 C0010 C0009
1033    LD      X0022.3
1034    OR      X0022.6
1035    MOVN    0001 C0009 G0010
1036    MOVN    0001 G0010 K0001
1037    LD      R0111.0
1038    CMP     0004 15 C0009 K0008.0
1039    CMP     0004 0 C0010 K0008.3
1040    LD      K0008.1
1041    OUT     Y0020.1
1042    LD      K0008.4
1043    OUT     Y0020.4
1044    SPE
1045    SP      P0010
1046    LD      X0020.5
1047    AND     X0020.7
1048    OUT     R0016.7
1049    LD      X0020.5
1050    ANI     F0214.0
1051    LD      X0020.7
1052    AND     F0214.0
1053    ORB
1054    ANI     R0016.7
1055    OUT     R0016.1
1056    LD      X0020.7
1057    ANI     F0214.0
1058    LD      X0020.5
1059    AND     F0214.0
1060    ORB
1061    ANI     R0016.7
1062    OUT     R0016.0
1063    SPE
1064    SP      P0011
1065    LD      X0020.4
1066    AND     X0021.0
1067    OUT     R0018.0
1068    LD      X0020.4
1069    ANI     F0214.1
1070    LD      X0021.0
1071    AND     F0214.1
1072    ORB
1073    ANI     R0018.0
1074    OUT     R0016.4
1075    LD      X0021.0
1076    ANI     F0214.1
1077    LD      X0020.4
1078    AND     F0214.1
1079    ORB
1080    ANI     R0018.0
1081    OUT     R0016.5
1082    SPE
1083    SP      P0012
1084    LD      X0020.3
1085    AND     X0021.1
1086    OUT     R0016.6
1087    LD      X0020.3
1088    ANI     F0214.2
1089    LD      X0021.1
1090    AND     F0214.2
1091    ORB
1092    ANI     R0016.6
1093    OUT     R0016.3
1094    LD      X0021.1
1095    ANI     F0214.2
1096    LD      X0020.3
1097    AND     F0214.2
1098    ORB
1099    ANI     R0016.6
1100    OUT     R0016.2
1101    SPE
1102    SP      P0013
1103    LD      X0020.2
1104    AND     X0021.2
1105    OUT     R0018.1
1106    LD      X0021.2
1107    ANI     F0214.3
1108    LD      X0020.2
1109    AND     F0214.3
1110    ORB
1111    ANI     R0018.1
1112    OUT     R0018.2
1113    LD      X0020.2
1114    ANI     F0214.3
1115    LD      X0021.2
1116    AND     F0214.3
1117    ORB
1118    ANI     R0018.1
1119    OUT     R0018.3
1120    SPE
1121    SP      P0014
1122    LD      X0020.1
1123    AND     X0025.6
1124    OUT     R0019.0
1125    LD      X0020.1
1126    ANI     F0214.4
1127    LD      X0025.6
1128    AND     F0214.4
1129    ORB
1130    ANI     R0019.0
1131    OUT     R0019.1
1132    LD      X0025.6
1133    ANI     F0214.4
1134    LD      X0020.1
1135    AND     F0214.4
1136    ORB
1137    ANI     R0019.0
1138    OUT     R0019.2
1139    SPE
1140    SP      P0015
1141    LD      R0307.2
1142    RST     R0307.7
1143    RST     R0307.6
1144    LDI     R0307.0
1145    ANI     R0307.6
1146    ANI     R0307.2
1147    SET     R0307.6
1148    LD      R0307.6
1149    TMRB    T0005 DT0022 R0307.1
1150    LD      R0307.1
1151    ANI     R0307.2
1152    OUT     Y0000.7
1153    LD      Y0000.7
1154    TMRB    T0004 DT0023 R0307.2
1155    SPE
1156    SP      P0016
1157    LD      X0021.6
1158    LD      R0032.0
1159    ANI     R0014.0
1160    ORB
1161    LD      R0119.2
1162    AND     R0014.0
1163    ORB
1164    CTRC    0000 R0270.0 C0008 1 R0014.0
1165    LD      R0014.0
1166    OUT     Y0000.1
1167    SPE
1168    SP      P0017
1169    LD      R0469.6
1170    ANI     R0469.7
1171    ANI     R0119.2
1172    ANI     R0270.0
1173    OR      X0021.6
1174    OR      R0032.0
1175    TMRB    T0006 DT0018 R0469.7
1176    OUT     R0469.6
1177    OUT     Y0000.1
1178    SPE
1179    SP      P0018
1180    LDI     R0800.1
1181    ANI     R0800.7
1182    TMRB    T0007 DT0016 R0800.0
1183    LD      X0021.6
1184    OR      R0800.7
1185    ANI     R0800.1
1186    OUT     R0800.7
1187    LD      R0800.0
1188    OR      R0800.7
1189    TMRB    T0008 DT0017 R0800.1
1190    LD      R0800.0
1191    OR      R0800.7
1192    OUT     Y0000.1
1193    SPE
1194    SP      P0019
1195    LD      X0018.0
1196    ANI     X0018.1
1197    ANI     X0018.2
1198    ANI     X0018.3
1199    ANI     X0018.4
1200    ANI     X0018.5
1201    ANI     X0019.3
1202    OUT     R0082.0
1203    LDI     X0018.0
1204    AND     X0018.1
1205    ANI     X0018.2
1206    ANI     X0018.3
1207    ANI     X0018.4
1208    ANI     X0018.5
1209    ANI     X0019.3
1210    OUT     R0082.1
1211    LDI     X0018.0
1212    ANI     X0018.1
1213    AND     X0018.2
1214    ANI     X0018.3
1215    ANI     X0018.4
1216    ANI     X0018.5
1217    ANI     X0019.3
1218    OUT     R0082.2
1219    LDI     X0018.0
1220    ANI     X0018.1
1221    ANI     X0018.2
1222    AND     X0018.3
1223    ANI     X0018.4
1224    ANI     X0018.5
1225    ANI     X0019.3
1226    OUT     R0082.3
1227    LDI     X0018.0
1228    ANI     X0018.1
1229    ANI     X0018.2
1230    ANI     X0018.3
1231    AND     X0018.4
1232    ANI     X0018.5
1233    ANI     X0019.3
1234    OUT     R0082.4
1235    LDI     X0018.0
1236    ANI     X0018.1
1237    ANI     X0018.2
1238    ANI     X0018.3
1239    ANI     X0018.4
1240    AND     X0018.5
1241    ANI     X0019.3
1242    OUT     R0082.5
1243    LD      R0082.0
1244    SET     G0043.0
1245    SET     G0043.1
1246    RST     G0043.2
1247    LD      R0082.1
1248    SET     G0043.0
1249    RST     G0043.1
1250    RST     G0043.2
1251    LD      R0082.2
1252    RST     G0043.0
1253    RST     G0043.1
1254    RST     G0043.2
1255    LD      R0082.4
1256    RST     G0043.0
1257    RST     G0043.1
1258    SET     G0043.2
1259    LD      R0082.5
1260    SET     G0043.0
1261    RST     G0043.1
1262    SET     G0043.2
1263    RST     G0043.7
1264    LD      R0082.3
1265    SET     G0043.0
1266    RST     G0043.1
1267    SET     G0043.2
1268    SET     G0043.7
1269    SPE
1270    SP      P0020
1271    LD      R0018.2
1272    LD      R0015.6
1273    AND     F0205.2
1274    ORB
1275    AND     F0004.5
1276    AND     R0466.3
1277    ANI     Y0022.4
1278    AND     G0130.3
1279    OUT     R0015.6
1280    LD      R0018.3
1281    LD      R0015.7
1282    AND     F0205.2
1283    ORB
1284    AND     F0004.5
1285    AND     R0466.3
1286    ANI     Y0022.4
1287    AND     G0130.3
1288    OUT     R0015.7
1289    LD      R0018.2
1290    OR      R0015.6
1291    AND     F0000.6
1292    AND     G0130.3
1293    OUT     G0100.3
1294    LD      R0018.3
1295    OR      R0015.7
1296    AND     F0000.6
1297    AND     G0130.3
1298    OUT     G0102.3
1299    LD      F0094.3
1300    OR      F0096.3
1301    OR      F0098.3
1302    OR      F0100.3
1303    OUT     Y0022.4
1304    SPE
1305    SP      P0021
1306    LD      R0019.1
1307    LD      R0019.4
1308    AND     F0205.2
1309    ORB
1310    AND     F0004.5
1311    AND     R0466.3
1312    AND     G0130.4
1313    OUT     R0019.4
1314    LD      R0019.2
1315    LD      R0019.5
1316    AND     F0205.2
1317    ORB
1318    AND     F0004.5
1319    AND     R0466.3
1320    AND     G0130.4
1321    OUT     R0019.5
1322    LD      R0019.2
1323    OR      R0019.5
1324    AND     F0000.6
1325    AND     G0130.4
1326    OUT     G0100.4
1327    LD      R0019.1
1328    OR      R0019.4
1329    AND     F0000.6
1330    AND     G0130.4
1331    OUT     G0102.4
1332    SPE
1333    SP      P0022
1334    LD      F0007.0
1335    DECB    0001 F0010 60 R0060
1336    LD      R0133.3
1337    OR      R0133.4
1338    SET     G0027.0
1339    RST     G0027.1
1340    SET     G0027.3
1341    LD      R0060.3
1342    OR      R0060.4
1343    SET     G0027.1
1344    RST     G0027.0
1345    SET     G0027.4
1346    LD      R0060.5
1347    AND     F0001.3
1348    OUT     R0062.0
1349    LD      R0060.5
1350    OUT     R0185.0
1351    LD      R0060.3
1352    AND     Y0003.4
1353    LD      R0060.4
1354    AND     Y0003.3
1355    ORB
1356    OUT     A0000.7
1357    LD      X0021.5
1358    ANI     R0017.0
1359    OUT     R0063.0
1360    LD      X0021.3
1361    ANI     R0017.0
1362    OUT     R0063.1
1363    LD      X0021.7
1364    ANI     R0017.0
1365    OUT     R0063.2
1366    LD      X0025.5
1367    LDI     R0017.0
1368    OR      K0010.4
1369    ANB
1370    AND     G0027.1
1371    OUT     R0064.0
1372    LDI     R0063.0
1373    ANI     R0062.0
1374    ANI     R0270.0
1375    ANI     F0009.4
1376    ANI     F0035.0
1377    OUT     R0065.0
1378    LD      R0063.2
1379    OR      R0060.3
1380    OR      R0076.0
1381    AND     R0065.0
1382    ANI     R0037.6
1383    ANI     R0006.0
1384    ANI     R0008.0
1385    ANI     Y0003.4
1386    OUT     R0076.0
1387    LD      R0064.0
1388    ANI     Y0002.1
1389    ANI     R0037.6
1390    ANI     R0076.0
1391    ANI     R0008.0
1392    AND     R0065.0
1393    OUT     R0076.1
1394    LD      R0076.0
1395    OR      R0076.1
1396    OUT     Y0003.3
1397    LD      R0060.4
1398    OR      R0063.1
1399    OR      R0077.0
1400    AND     R0065.0
1401    ANI     R0037.6
1402    ANI     R0006.0
1403    ANI     R0008.0
1404    ANI     Y0003.3
1405    OUT     R0077.0
1406    LD      R0077.0
1407    OUT     Y0003.4
1408    LD      Y0003.3
1409    OR      Y0003.4
1410    OUT     R0037.0
1411    LD      R0037.0
1412    SET     R0037.7
1413    LD      R0037.7
1414    CALL    P0023
1415    LD      R0060.3
1416    OR      R0060.4
1417    OR      R0060.5
1418    OUT     R0096.0
1419    SPE
1420    SP      P0023
1421    LD      R0037.2
1422    RST     R0037.7
1423    RST     R0037.6
1424    LDI     R0037.0
1425    ANI     R0037.6
1426    ANI     R0037.2
1427    SET     R0037.6
1428    LD      R0037.6
1429    TMRB    T0028 DT0022 R0037.1
1430    LD      R0037.1
1431    ANI     R0037.2
1432    OUT     Y0003.5
1433    LD      Y0003.5
1434    TMRB    T0021 DT0023 R0037.2
1435    SPE
1436    SP      P0024
1437    LD      F0007.0
1438    DECB    0001 F0010 40 R0040
1439    LD      R0040.1
1440    ANI     G0028.0
1441    ANI     G0028.1
1442    AND     X0001.6
1443    LD      R0040.2
1444    AND     G0028.0
1445    ANI     G0028.1
1446    AND     X0002.6
1447    ORB
1448    LD      R0040.3
1449    ANI     G0028.0
1450    AND     G0028.1
1451    AND     X0003.3
1452    ORB
1453    LD      R0040.4
1454    AND     G0028.0
1455    AND     G0028.1
1456    AND     X0003.4
1457    ORB
1458    ANI     R0044.5
1459    OUT     R0046.0
1460    LD      F0007.0
1461    ANI     R0046.6
1462    ANI     R0044.5
1463    OUT     G0033.7
1464    MOVN    0002 DT0031 R0042
1465    TMRB    T0032 DT0032 R0044.5
1466    LD      G0033.7
1467    MOVN    0001 R0042 G0032
1468    LD      R0043.0
1469    OUT     G0033.0
1470    LD      R0043.1
1471    OUT     G0033.1
1472    LD      R0043.2
1473    OUT     G0033.2
1474    LD      R0043.3
1475    OUT     G0033.3
1476    LD      R0111.0
1477    CALL    P0025
1478    LD      K0003.0
1479    OUT     G0028.0
1480    LD      K0003.1
1481    OUT     G0028.1
1482    LD      R0040.1
1483    AND     X0001.6
1484    LD      R0040.2
1485    AND     X0002.6
1486    ORB
1487    LD      R0040.3
1488    AND     X0003.3
1489    ORB
1490    LD      R0040.4
1491    AND     X0003.4
1492    ORB
1493    TMRB    T0033 DT0033 R0046.6
1494    LD      R0046.0
1495    OR      R0046.6
1496    OUT     R0046.7
1497    LD      R0040.1
1498    OR      R0040.2
1499    OR      R0040.3
1500    OR      R0040.4
1501    OUT     R0046.3
1502    LD      R0040.1
1503    ANI     X0001.6
1504    LD      R0040.2
1505    ANI     X0002.6
1506    ORB
1507    LD      R0040.3
1508    ANI     X0003.3
1509    ORB
1510    LD      R0040.4
1511    ANI     X0003.4
1512    ORB
1513    TMRB    T0034 DT0034 A0001.0
1514    SPE
1515    SP      P0025
1516    LD      R0040.1
1517    AND     R0044.5
1518    RST     K0003.0
1519    RST     K0003.1
1520    LD      R0040.2
1521    AND     R0044.5
1522    SET     K0003.0
1523    RST     K0003.1
1524    LD      R0040.3
1525    AND     R0044.5
1526    RST     K0003.0
1527    SET     K0003.1
1528    LD      R0040.4
1529    AND     R0044.5
1530    SET     K0003.0
1531    SET     K0003.1
1532    LDI     K0003.0
1533    ANI     K0003.1
1534    LD      K0012.0
1535    LDI     K0012.0
1536    ANI     X0001.6
1537    ORB
1538    ANB
1539    OUT     Y0001.0
1540    LD      K0003.0
1541    ANI     K0003.1
1542    LD      K0012.0
1543    LDI     K0012.0
1544    ANI     X0002.6
1545    ORB
1546    ANB
1547    OUT     Y0001.1
1548    LDI     K0003.0
1549    AND     K0003.1
1550    LD      K0012.0
1551    LDI     K0012.0
1552    ANI     X0003.3
1553    ORB
1554    ANB
1555    OUT     Y0001.2
1556    LD      K0003.0
1557    AND     K0003.1
1558    LD      K0012.0
1559    LDI     K0012.0
1560    ANI     X0003.4
1561    ORB
1562    ANB
1563    OUT     Y0001.3
1564    SPE
1565    SP      P0026
1566    LD      F0007.0
1567    DECB    0004 F0010 50 R0050
1568    LD      R0604.0
1569    OR      R0603.0
1570    OR      X0025.7
1571    OR      R0022.5
1572    AND     X0001.7
1573    OR      A0002.2
1574    ANI     F0001.1
1575    OUT     A0002.2
1576    LD      Y0000.4
1577    OR      Y0000.3
1578    OR      Y0005.3
1579    OR      Y0005.2
1580    LD      X0001.5
1581    OR      R0050.4
1582    OR      R0050.5
1583    ANB
1584    OR      A0002.3
1585    ANI     F0001.1
1586    OUT     A0002.3
1587    LDI     Y0000.3
1588    ANI     Y0000.4
1589    ANI     Y0005.3
1590    OUT     R0302.3
1591    LD      X0001.5
1592    AND     R0138.1
1593    OUT     R0011.2
1594    LD      R0050.5
1595    AND     R0011.4
1596    LD      R0050.4
1597    ANI     R0011.4
1598    ORB
1599    AND     R0302.3
1600    ALT     R0011.4
1601    LD      R0011.4
1602    OR      R0011.2
1603    OUT     Y0002.0
1604    LD      R0050.5
1605    ANI     X0002.0
1606    ANI     F0001.1
1607    ANI     R0011.4
1608    TMRB    T0030 DT0030 A0002.1
1609    LD      R0050.4
1610    ANI     X0001.7
1611    ANI     F0001.1
1612    AND     R0011.4
1613    TMRB    T0031 DT0030 A0002.0
1614    LD      R0050.4
1615    AND     R0011.4
1616    AND     X0001.7
1617    OUT     R0073.2
1618    LD      R0050.5
1619    ANI     R0011.4
1620    AND     X0002.0
1621    OUT     R0073.3
1622    LD      R0073.2
1623    OR      R0073.3
1624    OUT     R0073.7
1625    SPE
1626    SP      P0030
1627    LD      F0007.0
1628    DECB    0004 F0010 60 R0060
1629    LD      F0007.0
1630    DECB    0004 F0010 68 R0061
1631    LD      X0002.1
1632    OR      A0001.5
1633    ANI     F0001.1
1634    OUT     A0001.5
1635    LD      X0002.2
1636    OR      A0001.3
1637    ANI     F0001.1
1638    OUT     A0001.3
1639    RST     Y0001.6
1640    RST     Y0001.7
1641    LDI     X0000.2
1642    OR      A0001.1
1643    ANI     K0011.1
1644    ANI     F0001.1
1645    OUT     A0001.1
1646    LD      R0111.0
1647    CALL    P0031
1648    LD      R0138.1
1649    CALL    P0032
1650    LD      R0335.0
1651    CALL    P0033
1652    LD      R0111.0
1653    CALL    P0036
1654    LD      R0111.0
1655    CALL    P0037
1656    LDI     R0001.0
1657    CALL    P0038
1658    LD      K0011.2
1659    AND     X0005.2
1660    AND     Y0022.5
1661    ORI     K0011.2
1662    CALL    P0039
1663    LDI     X0001.2
1664    AND     R0335.0
1665    ORI     R0335.0
1666    AND     K0011.0
1667    ORI     K0011.0
1668    OUT     G0130.0
1669    LDI     X0001.2
1670    AND     R0335.0
1671    ORI     R0335.0
1672    AND     K0011.0
1673    ORI     K0011.0
1674    OUT     G0130.1
1675    LDI     X0001.2
1676    OR      F0003.6
1677    AND     K0011.0
1678    ORI     K0011.0
1679    OUT     G0130.2
1680    LDI     X0001.2
1681    AND     R0335.0
1682    ORI     R0335.0
1683    AND     K0011.0
1684    ORI     K0011.0
1685    OUT     G0130.3
1686    LDI     X0001.2
1687    AND     R0335.0
1688    ORI     R0335.0
1689    AND     K0011.0
1690    ORI     K0011.0
1691    OUT     G0130.4
1692    LD      R0060.5
1693    ANI     R0020.0
1694    LD      R0060.6
1695    ANI     R0020.6
1696    ORB
1697    LD      R0061.0
1698    ANI     R0020.1
1699    ORB
1700    LD      R0061.1
1701    ANI     R0020.4
1702    ORB
1703    LD      R0061.2
1704    ANI     R0020.5
1705    ORB
1706    TMRB    T0025 DT0025 R0127.0
1707    LD      R0127.0
1708    OR      A0001.6
1709    ANI     F0001.1
1710    OUT     A0001.6
1711    LD      R0020.0
1712    OR      R0020.1
1713    OR      R0020.4
1714    OR      R0020.5
1715    OR      R0020.6
1716    OUT     R0020.7
1717    SPE
1718    SP      P0031
1719    LD      X0022.0
1720    AND     X0000.6
1721    AND     F0004.5
1722    SET     Y0001.6
1723    SET     R0126.0
1724    LD      F0001.1
1725    LD      R0126.0
1726    AND     Y0001.6
1727    ANI     F0004.5
1728    ORB
1729    LD      Y0001.6
1730    AND     F0004.5
1731    ANI     X0000.6
1732    ORB
1733    RST     Y0001.6
1734    RST     R0126.0
1735    LD      X0000.0
1736    AND     F0004.5
1737    RST     Y0001.6
1738    RST     R0126.0
1739    MOVN    0001 1 D0409
1740    MOVN    0001 1 D0408
1741    MOVN    0001 1 C0022
1742    MOVN    0001 1 C0023
1743    MOVN    0001 1 C0021
1744    SPE
1745    SP      P0032
1746    LD      X0018.6
1747    AND     K0021.0
1748    LD      X0022.0
1749    ANI     K0021.0
1750    ORB
1751    DIFU    R0008.7
1752    SET     R0008.2
1753    LD      R0008.7
1754    MOVN    0001 D0409 C0021
1755    CTRC    0010 R0003.7 C0021 F0207 R0003.7
1756    MOVN    0001 C0021 D0408
1757    LD      X0018.7
1758    AND     R0335.1
1759    AND     K0021.0
1760    DIFU    R0008.6
1761    SET     R0008.3
1762    LD      R0008.6
1763    MOVN    0001 D0409 C0021
1764    CTRC    0011 R0007.3 C0021 DC0001 R0007.3
1765    MOVN    0001 C0021 D0408
1766    SPE
1767    SP      P0033
1768    LD      F0007.3
1769    CALL    P0035
1770    TMRB    T0017 50 R0008.5
1771    SET     R0276.0
1772    LD      F0007.3
1773    AND     R0008.5
1774    OUT     R0211.0
1775    LD      R0276.0
1776    CMP     0001 F0026 D0410 R0007.4
1777    LD      R0276.0
1778    CMP     0001 D0408 D0409 R0000.3
1779    LD      R0007.5
1780    OUT     G0054.2
1781    LD      R0000.4
1782    AND     R0276.0
1783    SET     G0054.0
1784    LD      R0007.5
1785    OR      R0000.4
1786    ANI     Y0001.6
1787    ANI     Y0001.7
1788    OR      F0001.1
1789    RST     R0276.0
1790    SPE
1791    SP      P0034
1792    LD      R0111.0
1793    MOVN    0001 D0410 D0406
1794    LD      R0111.0
1795    CMP     0001 D0409 1 R0151.0
1796    LD      R0151.1
1797    MOVN    0001 D0411 D0410
1798    MOVN    0001 D0406 D0411
1799    LD      R0111.0
1800    CMP     0001 D0409 2 R0151.4
1801    LD      R0151.5
1802    MOVN    0001 D0412 D0410
1803    MOVN    0001 D0406 D0412
1804    LD      R0111.0
1805    CMP     0001 D0409 3 R0152.0
1806    LD      R0152.1
1807    MOVN    0001 D0413 D0410
1808    MOVN    0001 D0406 D0413
1809    LD      R0111.0
1810    CMP     0001 D0409 4 R0152.4
1811    LD      R0152.5
1812    MOVN    0001 D0414 D0410
1813    MOVN    0001 D0406 D0414
1814    LD      R0111.0
1815    CMP     0001 D0409 5 R0153.0
1816    LD      R0153.1
1817    MOVN    0001 D0415 D0410
1818    MOVN    0001 D0406 D0415
1819    LD      R0111.0
1820    CMP     0001 D0409 6 R0153.4
1821    LD      R0153.5
1822    MOVN    0001 D0416 D0410
1823    MOVN    0001 D0406 D0416
1824    LD      R0111.0
1825    CMP     0001 D0409 7 R0154.0
1826    LD      R0154.1
1827    MOVN    0001 D0417 D0410
1828    MOVN    0001 D0406 D0417
1829    LD      R0111.0
1830    CMP     0001 D0409 8 R0154.4
1831    LD      R0154.5
1832    MOVN    0001 D0418 D0410
1833    MOVN    0001 D0406 D0418
1834    LD      R0111.0
1835    CMP     0001 D0409 9 R0155.0
1836    LD      R0155.1
1837    MOVN    0001 D0419 D0410
1838    MOVN    0001 D0406 D0419
1839    LD      R0111.0
1840    CMP     0001 D0409 10 R0155.4
1841    LD      R0155.5
1842    MOVN    0001 D0420 D0410
1843    MOVN    0001 D0406 D0420
1844    LD      R0111.0
1845    CMP     0001 D0409 11 R0156.0
1846    LD      R0156.1
1847    MOVN    0001 D0421 D0410
1848    MOVN    0001 D0406 D0421
1849    LD      R0111.0
1850    CMP     0001 D0409 12 R0156.4
1851    LD      R0156.5
1852    MOVN    0001 D0422 D0410
1853    MOVN    0001 D0406 D0422
1854    LD      R0111.0
1855    CMP     0001 D0409 13 R0157.0
1856    LD      R0157.1
1857    MOVN    0001 D0423 D0410
1858    MOVN    0001 D0406 D0423
1859    LD      R0111.0
1860    CMP     0001 D0409 14 R0157.4
1861    LD      R0157.5
1862    MOVN    0001 D0424 D0410
1863    MOVN    0001 D0406 D0424
1864    LD      R0111.0
1865    CMP     0001 D0409 15 R0158.0
1866    LD      R0158.1
1867    MOVN    0001 D0425 D0410
1868    MOVN    0001 D0406 D0425
1869    LD      R0111.0
1870    CMP     0001 D0409 16 R0158.4
1871    LD      R0158.5
1872    MOVN    0001 D0426 D0410
1873    MOVN    0001 D0406 D0426
1874    LD      R0111.0
1875    CMP     0001 D0409 17 R0159.0
1876    LD      R0159.1
1877    MOVN    0001 D0427 D0410
1878    MOVN    0001 D0406 D0427
1879    LD      R0111.0
1880    CMP     0001 D0409 18 R0159.4
1881    LD      R0159.5
1882    MOVN    0001 D0428 D0410
1883    MOVN    0001 D0406 D0428
1884    LD      R0111.0
1885    CMP     0001 D0409 19 R0160.0
1886    LD      R0160.1
1887    MOVN    0001 D0429 D0410
1888    MOVN    0001 D0406 D0429
1889    LD      R0111.0
1890    CMP     0001 D0409 20 R0160.4
1891    LD      R0160.5
1892    MOVN    0001 D0430 D0410
1893    MOVN    0001 D0406 D0430
1894    LD      R0111.0
1895    CMP     0001 D0409 21 R0161.0
1896    LD      R0161.1
1897    MOVN    0001 D0431 D0410
1898    MOVN    0001 D0406 D0431
1899    LD      R0111.0
1900    CMP     0001 D0409 22 R0161.4
1901    LD      R0161.5
1902    MOVN    0001 D0432 D0410
1903    MOVN    0001 D0406 D0432
1904    LD      R0111.0
1905    CMP     0001 D0409 23 R0162.0
1906    LD      R0162.1
1907    MOVN    0001 D0433 D0410
1908    MOVN    0001 D0406 D0433
1909    LD      R0111.0
1910    CMP     0001 D0409 24 R0162.4
1911    LD      R0162.5
1912    MOVN    0001 D0434 D0410
1913    MOVN    0001 D0406 D0434
1914    LD      R0111.0
1915    CMP     0001 D0409 25 R0163.1
1916    LD      R0163.2
1917    MOVN    0001 D0435 D0410
1918    MOVN    0001 D0406 D0435
1919    LD      R0111.0
1920    CMP     0001 D0409 26 R0163.4
1921    LD      R0163.5
1922    MOVN    0001 D0436 D0410
1923    MOVN    0001 D0406 D0436
1924    LD      R0111.0
1925    CMP     0001 D0409 27 R0164.1
1926    LD      R0164.2
1927    MOVN    0001 D0437 D0410
1928    MOVN    0001 D0406 D0437
1929    LD      R0111.0
1930    CMP     0001 D0409 28 R0164.4
1931    LD      R0164.5
1932    MOVN    0001 D0438 D0410
1933    MOVN    0001 D0406 D0438
1934    LD      R0111.0
1935    CMP     0001 D0409 29 R0165.1
1936    LD      R0165.2
1937    MOVN    0001 D0439 D0410
1938    MOVN    0001 D0406 D0439
1939    LD      R0111.0
1940    CMP     0001 D0409 30 R0165.4
1941    LD      R0165.5
1942    MOVN    0001 D0440 D0410
1943    MOVN    0001 D0406 D0440
1944    LD      R0111.0
1945    CMP     0001 D0409 31 R0166.1
1946    LD      R0166.2
1947    MOVN    0001 D0441 D0410
1948    MOVN    0001 D0406 D0441
1949    LD      R0111.0
1950    CMP     0001 D0409 32 R0166.4
1951    LD      R0166.5
1952    MOVN    0001 D0442 D0410
1953    MOVN    0001 D0406 D0442
1954    SPE
1955    SP      P0035
1956    LD      R0111.0
1957    CMP     0001 F0026 D0411 R0101.0
1958    LD      R0101.1
1959    MOVN    0001 1 D0408
1960    LD      R0111.0
1961    CMP     0001 F0026 D0412 R0101.4
1962    LD      R0101.5
1963    MOVN    0001 2 D0408
1964    LD      R0111.0
1965    CMP     0001 F0026 D0413 R0102.0
1966    LD      R0102.1
1967    MOVN    0001 3 D0408
1968    LD      R0111.0
1969    CMP     0001 F0026 D0414 R0102.4
1970    LD      R0102.5
1971    MOVN    0001 4 D0408
1972    LD      R0111.0
1973    CMP     0001 F0026 D0415 R0103.0
1974    LD      R0103.1
1975    MOVN    0001 5 D0408
1976    LD      R0111.0
1977    CMP     0001 F0026 D0416 R0103.4
1978    LD      R0103.5
1979    MOVN    0001 6 D0408
1980    LD      R0111.0
1981    CMP     0001 F0026 D0417 R0104.0
1982    LD      R0104.1
1983    MOVN    0001 7 D0408
1984    LD      R0111.0
1985    CMP     0001 F0026 D0418 R0104.4
1986    LD      R0104.5
1987    MOVN    0001 8 D0408
1988    LD      R0111.0
1989    CMP     0001 F0026 D0419 R0105.0
1990    LD      R0105.1
1991    MOVN    0001 9 D0408
1992    LD      R0111.0
1993    CMP     0001 F0026 D0420 R0105.4
1994    LD      R0105.5
1995    MOVN    0001 10 D0408
1996    LD      R0111.0
1997    CMP     0001 F0026 D0421 R0106.0
1998    LD      R0106.1
1999    MOVN    0001 11 D0408
2000    LD      R0111.0
2001    CMP     0001 F0026 D0422 R0106.4
2002    LD      R0106.5
2003    MOVN    0001 12 D0408
2004    LD      R0111.0
2005    CMP     0001 F0026 D0423 R0107.0
2006    LD      R0107.1
2007    MOVN    0001 13 D0408
2008    LD      R0111.0
2009    CMP     0001 F0026 D0424 R0107.4
2010    LD      R0107.5
2011    MOVN    0001 14 D0408
2012    LD      R0111.0
2013    CMP     0001 F0026 D0425 R0108.0
2014    LD      R0108.1
2015    MOVN    0001 15 D0408
2016    LD      R0111.0
2017    CMP     0001 F0026 D0426 R0108.4
2018    LD      R0108.5
2019    MOVN    0001 16 D0408
2020    LD      R0111.0
2021    CMP     0001 F0026 D0427 R0109.0
2022    LD      R0109.1
2023    MOVN    0001 17 D0408
2024    LD      R0111.0
2025    CMP     0001 F0026 D0428 R0109.4
2026    LD      R0109.5
2027    MOVN    0001 18 D0408
2028    LD      R0111.0
2029    CMP     0001 F0026 D0429 R0110.0
2030    LD      R0110.1
2031    MOVN    0001 19 D0408
2032    LD      R0111.0
2033    CMP     0001 F0026 D0430 R0110.4
2034    LD      R0110.5
2035    MOVN    0001 20 D0408
2036    LD      R0111.0
2037    CMP     0001 F0026 D0431 R0113.0
2038    LD      R0113.1
2039    MOVN    0001 21 D0408
2040    LD      R0111.0
2041    CMP     0001 F0026 D0432 R0112.4
2042    LD      R0112.5
2043    MOVN    0001 22 D0408
2044    LD      R0111.0
2045    CMP     0001 F0026 D0433 R0114.0
2046    LD      R0114.1
2047    MOVN    0001 23 D0408
2048    LD      R0111.0
2049    CMP     0001 F0026 D0434 R0114.4
2050    LD      R0114.5
2051    MOVN    0001 24 D0408
2052    LD      R0111.0
2053    CMP     0001 F0026 D0435 R0115.1
2054    LD      R0115.2
2055    MOVN    0001 25 D0408
2056    LD      R0111.0
2057    CMP     0001 F0026 D0436 R0115.4
2058    LD      R0115.5
2059    MOVN    0001 26 D0408
2060    LD      R0111.0
2061    CMP     0001 F0026 D0437 R0116.1
2062    LD      R0116.2
2063    MOVN    0001 27 D0408
2064    LD      R0111.0
2065    CMP     0001 F0026 D0438 R0116.4
2066    LD      R0116.5
2067    MOVN    0001 28 D0408
2068    LD      R0111.0
2069    CMP     0001 F0026 D0439 R0117.1
2070    LD      R0117.2
2071    MOVN    0001 29 D0408
2072    LD      R0111.0
2073    CMP     0001 F0026 D0440 R0117.4
2074    LD      R0117.5
2075    MOVN    0001 30 D0408
2076    LD      R0111.0
2077    CMP     0001 F0026 D0441 R0118.1
2078    LD      R0118.2
2079    MOVN    0001 31 D0408
2080    LD      R0111.0
2081    CMP     0001 F0026 D0442 R0118.4
2082    LD      R0118.5
2083    MOVN    0001 32 D0408
2084    SPE
2085    SP      P0036
2086    LD      R0276.0
2087    OR      R0008.2
2088    OR      R0008.3
2089    OR      R0001.0
2090    ANI     X0000.6
2091    OR      A0001.4
2092    ANI     F0001.1
2093    OUT     A0001.4
2094    RST     Y0001.6
2095    RST     Y0001.7
2096    LD      R0276.0
2097    OR      R0008.2
2098    OR      R0008.3
2099    ANI     R0001.0
2100    AND     X0000.6
2101    SET     R0001.0
2102    OUT     R0001.1
2103    RST     R0276.0
2104    LD      R0001.1
2105    CALL    P0047
2106    LDI     R0007.0
2107    ANI     Y0001.7
2108    AND     R0001.1
2109    ANI     A0001.4
2110    SET     Y0001.6
2111    RST     Y0001.7
2112    LD      R0007.0
2113    ANI     Y0001.6
2114    AND     R0001.1
2115    ANI     A0001.4
2116    SET     Y0001.7
2117    RST     Y0001.6
2118    SPE
2119    SP      P0037
2120    LD      X0000.4
2121    ANI     R0078.0
2122    OUT     R0041.2
2123    LD      X0000.4
2124    OUT     R0078.0
2125    RST     K0003.6
2126    RST     K0003.7
2127    LDI     X0000.4
2128    AND     Y0001.6
2129    SET     K0003.6
2130    LDI     X0000.4
2131    AND     Y0001.7
2132    SET     K0003.7
2133    LD      R0041.2
2134    AND     Y0001.6
2135    LD      K0003.6
2136    AND     Y0001.7
2137    AND     R0001.1
2138    ORB
2139    CTRC    0010 R0003.2 C0022 DC0001 R0006.1
2140    MOVN    0001 C0022 C0023
2141    LD      R0041.2
2142    AND     Y0001.7
2143    LD      K0003.7
2144    AND     Y0001.6
2145    AND     R0001.1
2146    ORB
2147    CTRC    0011 R0003.2 C0023 DC0001 R0006.2
2148    MOVN    0001 C0023 C0022
2149    LD      R0041.2
2150    LD      K0003.6
2151    AND     R0001.1
2152    ORB
2153    LD      K0003.7
2154    AND     R0001.1
2155    ORB
2156    LD      Y0001.6
2157    OR      Y0001.7
2158    ANB
2159    MOVN    0001 C0022 D0409
2160    LD      Y0001.6
2161    OR      Y0001.7
2162    CMP     0001 D0409 D0408 R0001.5
2163    OUT     Y0019.0
2164    TMRB    T0014 DT0028 A0001.2
2165    LD      R0001.6
2166    OR      F0001.1
2167    OR      A0001.2
2168    ANI     F0004.5
2169    RST     Y0001.7
2170    RST     Y0001.6
2171    RST     R0001.0
2172    DIFU    R0177.0
2173    LDI     R0001.0
2174    AND     R0177.0
2175    ANI     F0001.1
2176    ANI     A0001.2
2177    SET     G0054.0
2178    LDI     R0001.0
2179    AND     R0008.2
2180    AND     R0177.0
2181    RST     R0008.2
2182    LDI     R0001.0
2183    AND     R0008.3
2184    AND     R0177.0
2185    RST     R0008.3
2186    SPE
2187    SP      P0038
2188    LD      R0030.4
2189    AND     R0335.1
2190    SET     R0007.2
2191    LD      R0060.5
2192    OR      R0007.2
2193    ANI     X0000.7
2194    ANI     X0001.2
2195    ANI     Y0001.6
2196    ANI     Y0001.7
2197    OUT     Y0001.4
2198    LD      X0000.7
2199    AND     R0060.5
2200    OUT     R0020.0
2201    LD      X0000.7
2202    OR      F0001.1
2203    AND     R0007.2
2204    RST     R0007.2
2205    LD      R0030.3
2206    AND     R0335.1
2207    SET     R0007.1
2208    LD      R0060.6
2209    OR      R0007.1
2210    ANI     X0000.6
2211    ANI     X0001.2
2212    ANI     Y0001.6
2213    ANI     Y0001.7
2214    OUT     Y0001.5
2215    LD      X0000.6
2216    AND     R0060.6
2217    OUT     R0020.6
2218    RST     G0054.0
2219    LD      X0000.6
2220    OR      F0001.1
2221    AND     R0007.1
2222    RST     R0007.1
2223    SPE
2224    SP      P0039
2225    LD      X0001.0
2226    DIFD    R0076.0
2227    LD      X0001.1
2228    DIFD    R0076.1
2229    LD      R0061.0
2230    ANI     R0076.0
2231    ANI     R0076.1
2232    ANI     R0020.1
2233    AND     X0000.7
2234    LD      R0061.1
2235    ANI     R0076.0
2236    ANI     R0076.1
2237    ANI     R0020.4
2238    LD      X0001.7
2239    OR      K0011.3
2240    ANB
2241    ORB
2242    LD      R0061.2
2243    ANI     R0020.5
2244    AND     X0001.2
2245    LD      X0002.0
2246    OR      K0011.3
2247    ANB
2248    ORB
2249    OUT     R0076.3
2250    LD      R0076.3
2251    ANI     A0001.5
2252    ANI     F0001.1
2253    OUT     Y0002.1
2254    LDI     Y0002.1
2255    AND     R0061.0
2256    ANI     X0001.0
2257    ANI     X0001.1
2258    OUT     R0020.1
2259    LDI     Y0002.1
2260    AND     R0061.1
2261    ANI     X0001.0
2262    ANI     X0001.1
2263    OUT     R0020.4
2264    DIFU    R0000.1
2265    LD      R0000.1
2266    CALL    P0034
2267    MOVN    0001 D0410 G0201
2268    LDI     Y0002.1
2269    AND     R0061.2
2270    ANI     X0001.2
2271    OUT     R0020.5
2272    SPE
2273    SP      P0040
2274    LD      F0007.0
2275    DECB    0004 F0010 60 R0060
2276    LDI     R0001.1
2277    AND     F0003.3
2278    ANI     Y0001.6
2279    ANI     F0000.5
2280    ANI     Y0001.7
2281    OUT     R0278.5
2282    LD      R0278.5
2283    MOVN    0001 D0409 C0023
2284    MOVN    0001 D0409 C0022
2285    LD      X0002.2
2286    OR      A0001.3
2287    ANI     F0001.1
2288    OUT     A0001.3
2289    RST     Y0001.6
2290    RST     Y0001.7
2291    LDI     X0000.2
2292    OR      A0001.1
2293    ANI     F0001.1
2294    ANI     K0011.1
2295    OUT     A0001.1
2296    LDI     R0060.0
2297    CALL    P0041
2298    LDI     R0060.0
2299    AND     R0138.1
2300    CALL    P0042
2301    LD      R0335.0
2302    CALL    P0043
2303    LD      F0054.0
2304    AND     K0011.2
2305    ORI     K0011.2
2306    CALL    P0044
2307    LD      R0111.0
2308    CALL    P0045
2309    LD      R0111.0
2310    CALL    P0046
2311    LD      R0060.1
2312    MOVN    0001 D0409 G0201
2313    OUT     R0020.1
2314    LD      R0060.0
2315    ANI     R0020.0
2316    LD      R0060.5
2317    ANI     R0020.5
2318    ORB
2319    LD      R0060.6
2320    ANI     R0020.6
2321    ORB
2322    TMRB    T0026 DT0026 R0127.1
2323    LD      R0127.1
2324    OR      A0002.4
2325    ANI     F0001.1
2326    OUT     A0002.4
2327    LD      R0020.0
2328    OR      R0020.1
2329    OR      R0020.5
2330    OR      R0020.6
2331    OUT     R0020.7
2332    SPE
2333    SP      P0041
2334    LD      X0022.0
2335    AND     X0000.6
2336    AND     F0004.5
2337    SET     Y0001.6
2338    SET     R0126.1
2339    LD      F0001.1
2340    LD      R0126.1
2341    AND     Y0001.6
2342    ANI     F0004.5
2343    ORB
2344    LDI     X0000.6
2345    AND     F0004.5
2346    AND     Y0001.6
2347    ORB
2348    RST     Y0001.6
2349    RST     R0126.1
2350    LD      X0000.0
2351    AND     F0004.5
2352    RST     Y0001.6
2353    RST     R0126.1
2354    MOVN    0001 1 D0409
2355    MOVN    0001 1 D0408
2356    MOVN    0001 1 C0022
2357    MOVN    0001 1 C0023
2358    MOVN    0001 1 C0021
2359    SPE
2360    SP      P0042
2361    LD      R0030.1
2362    AND     K0021.0
2363    LD      X0022.5
2364    ANI     K0021.0
2365    ORB
2366    DIFU    R0008.7
2367    SET     R0008.2
2368    LD      R0008.7
2369    MOVN    0001 D0409 C0021
2370    CTRC    0010 R0003.7 C0021 DC0001 R0003.7
2371    MOVN    0001 C0021 D0408
2372    LD      R0030.2
2373    AND     K0021.0
2374    DIFU    R0008.6
2375    SET     R0008.3
2376    LD      R0008.6
2377    MOVN    0001 D0409 C0021
2378    CTRC    0011 R0007.3 C0021 DC0001 R0007.3
2379    MOVN    0001 C0021 D0408
2380    SPE
2381    SP      P0043
2382    LD      F0007.3
2383    TMRB    T0020 50 R0008.5
2384    MOVN    0001 F0026 D0408
2385    RST     G0054.0
2386    LD      F0007.3
2387    AND     R0008.5
2388    OUT     R0211.3
2389    LD      F0007.3
2390    CMP     0001 D0408 D0409 R0007.5
2391    LD      R0007.6
2392    SET     G0054.0
2393    SPE
2394    SP      P0044
2395    LD      X0003.4
2396    OR      R0128.0
2397    AND     R0355.1
2398    ANI     Y0001.7
2399    ANI     X0000.7
2400    ANI     F0001.1
2401    ANI     Y0001.6
2402    OUT     R0128.0
2403    LD      R0060.5
2404    OR      R0128.0
2405    ANI     Y0001.6
2406    ANI     Y0001.7
2407    ANI     X0000.7
2408    ANI     A0002.4
2409    ANI     F0001.1
2410    OUT     Y0001.4
2411    LD      X0000.7
2412    AND     R0060.5
2413    OUT     R0020.5
2414    LD      X0003.3
2415    OR      R0128.1
2416    AND     R0355.1
2417    ANI     Y0001.7
2418    ANI     X0000.7
2419    ANI     F0001.1
2420    ANI     Y0001.6
2421    OUT     R0128.1
2422    LD      R0060.6
2423    OR      R0128.1
2424    ANI     Y0001.6
2425    ANI     Y0001.7
2426    ANI     X0000.6
2427    ANI     A0002.4
2428    ANI     F0001.1
2429    OUT     Y0001.5
2430    LD      X0000.6
2431    AND     R0060.6
2432    OUT     R0020.6
2433    SPE
2434    SP      P0045
2435    LD      R0060.0
2436    OR      R0008.2
2437    OR      R0008.3
2438    ANI     R0001.1
2439    LD      F0098.2
2440    OR      K0011.4
2441    ANB
2442    SET     R0001.1
2443    OUT     R0001.0
2444    LD      R0001.0
2445    CALL    P0047
2446    LDI     R0007.0
2447    ANI     Y0001.7
2448    ANI     A0001.4
2449    AND     R0001.0
2450    SET     Y0001.6
2451    RST     Y0001.7
2452    LD      R0007.0
2453    ANI     Y0001.6
2454    ANI     A0001.4
2455    AND     R0001.0
2456    SET     Y0001.7
2457    RST     Y0001.6
2458    SPE
2459    SP      P0046
2460    LD      X0000.4
2461    ANI     R0078.0
2462    OUT     R0085.1
2463    LD      X0000.4
2464    OUT     R0078.0
2465    RST     K0003.6
2466    RST     K0003.7
2467    LDI     X0000.4
2468    AND     Y0001.6
2469    SET     K0003.6
2470    LDI     X0000.4
2471    AND     Y0001.7
2472    SET     K0003.7
2473    LD      R0085.1
2474    AND     Y0001.6
2475    LD      K0003.6
2476    AND     Y0001.7
2477    AND     R0001.0
2478    ORB
2479    CTRC    0010 R0086.0 C0022 DC0001 R0086.1
2480    MOVN    0001 C0022 C0023
2481    LD      R0085.1
2482    AND     Y0001.7
2483    LD      K0003.7
2484    AND     Y0001.6
2485    AND     R0001.0
2486    ORB
2487    CTRC    0011 R0087.0 C0022 DC0001 R0087.1
2488    MOVN    0001 C0022 C0023
2489    LD      R0085.1
2490    LD      K0003.6
2491    AND     R0001.0
2492    ORB
2493    LD      K0003.7
2494    AND     R0001.0
2495    ORB
2496    LD      Y0001.6
2497    OR      Y0001.7
2498    ANB
2499    MOVN    0001 C0022 D0409
2500    LD      Y0001.6
2501    OR      Y0001.7
2502    CMP     0001 D0408 D0409 R0000.5
2503    TMRB    T0030 DT0028 A0001.2
2504    OUT     Y0019.0
2505    LD      R0000.6
2506    OR      F0001.1
2507    ANI     F0004.5
2508    RST     Y0001.6
2509    RST     Y0001.7
2510    OUT     R0020.0
2511    RST     R0001.1
2512    LDI     R0001.1
2513    LD      R0008.2
2514    OR      R0008.3
2515    ANB
2516    RST     R0008.2
2517    RST     R0008.3
2518    SPE
2519    SP      P0047
2520    LD      R0111.0
2521    CMP     0001 F0207 8 R0130.1
2522    LD      R0130.2
2523    ROTB    1100 0008 0001 D0409 D0408 R0009 R0007.0
2524    LD      R0111.0
2525    CMP     0001 F0207 16 R0130.4
2526    LD      R0130.5
2527    ROTB    1100 0016 0001 D0409 D0408 R0009 R0007.0
2528    LD      R0111.0
2529    CMP     0001 F0207 20 R0131.1
2530    LD      R0131.2
2531    ROTB    1100 0020 0001 D0409 D0408 R0009 R0007.0
2532    LD      R0111.0
2533    CMP     0001 F0207 24 R0131.4
2534    LD      R0131.5
2535    ROTB    1100 0024 0001 D0409 D0408 R0009 R0007.0
2536    LD      R0111.0
2537    CMP     0001 F0207 32 R0132.1
2538    LD      R0132.2
2539    ROTB    1100 0032 0001 D0409 D0408 R0009 R0007.0
2540    SPE
2541    SP      P0050
2542    LD      K0015.7
2543    OUT     G0114.3
2544    OUT     G0114.4
2545    OUT     G0116.3
2546    OUT     G0116.4
2547    LD      X0002.7
2548    AND     K0015.0
2549    LDI     X0002.7
2550    ANI     K0015.0
2551    ORB
2552    OUT     G0116.0
2553    LD      X0003.0
2554    AND     K0015.0
2555    LDI     X0003.0
2556    ANI     K0015.0
2557    ORB
2558    OUT     G0114.0
2559    LD      X0003.1
2560    AND     K0015.0
2561    LDI     X0003.1
2562    ANI     K0015.0
2563    ORB
2564    OUT     G0116.1
2565    LD      X0003.2
2566    AND     K0015.0
2567    LDI     X0003.2
2568    ANI     K0015.0
2569    ORB
2570    OUT     G0114.1
2571    LD      X0003.6
2572    AND     K0015.0
2573    LDI     X0003.6
2574    ANI     K0015.0
2575    ORB
2576    OUT     G0116.2
2577    LD      X0003.7
2578    AND     K0015.0
2579    LDI     X0003.7
2580    ANI     K0015.0
2581    ORB
2582    OUT     G0114.2
2583    SPE
END_PLC_ORGANIZATION

PLC_INFO
TOTALTIPS	4
GSK
1AA5
2012.04.10
GSK980MDa Standard Ladder
END_PLC_INFO

PLC_ALARM
TOTALTIPS	18
0000	5000	illegal M code
0003	5003	M03¡¢M04 error
0002	5002	M29 overtime
0004	5004	M19,detect vpo(X5.2) signal  too long
0013	5013	disc tool arm motor overload
0005	5005	M14,detect vp(X5.0) signal  too long
0009	5009	cylinder pressure is low
0010	5010	cutter rotation time is too long
0011	5011	cutter motor overload
0012	5012	cutter rotates,the pocket in place must be level
0016	5016	checkout release tool
0017	5017	checkout the clamping tool
0018	5018	release the tool,the spindle can't not rotate
0019	5019	spindle rotation,can't release the tool
0007	5007	M63¡¢M64 error
0008	5008	spindle mechanical gears changed is too long
0014	5014	disc tool M68¡¢M69¡¢M65¡¢M66¡¢M70 execution timeout,pealse check the complete signal
0020	5020	armless type ATC M65¡¢M66¡¢M60 execution timeout,pealse check the complete signal
END_PLC_ALARM

PLC_INIT_D
TOTALTIPS	1000
0001	0
0002	0
0003	0
0004	0
0005	0
0006	0
0007	0
0008	0
0009	0
0010	0
0011	0
0012	0
0013	0
0014	0
0015	0
0016	0
0017	0
0018	0
0019	0
0020	0
0021	0
0022	0
0023	0
0024	0
0025	0
0026	0
0027	0
0028	0
0029	0
0030	0
0031	0
0032	0
0033	0
0034	0
0035	0
0036	0
0037	0
0038	0
0039	0
0040	0
0041	0
0042	0
0043	0
0044	0
0045	0
0046	0
0047	0
0048	0
0049	0
0050	0
0051	0
0052	0
0053	0
0054	0
0055	0
0056	0
0057	0
0058	0
0059	0
0060	0
0061	0
0062	0
0063	0
0064	0
0065	0
0066	0
0067	0
0068	0
0069	0
0070	0
0071	0
0072	0
0073	0
0074	0
0075	0
0076	0
0077	0
0078	0
0079	0
0080	0
0081	0
0082	0
0083	0
0084	0
0085	0
0086	0
0087	0
0088	0
0089	0
0090	0
0091	0
0092	0
0093	0
0094	0
0095	0
0096	0
0097	0
0098	0
0099	0
0100	0
0101	0
0102	0
0103	0
0104	0
0105	0
0106	0
0107	0
0108	0
0109	0
0110	0
0111	0
0112	0
0113	0
0114	0
0115	0
0116	0
0117	0
0118	0
0119	0
0120	0
0121	0
0122	0
0123	0
0124	0
0125	0
0126	0
0127	0
0128	0
0129	0
0130	0
0131	0
0132	0
0133	0
0134	0
0135	0
0136	0
0137	0
0138	0
0139	0
0140	0
0141	0
0142	0
0143	0
0144	0
0145	0
0146	0
0147	0
0148	0
0149	0
0150	0
0151	0
0152	0
0153	0
0154	0
0155	0
0156	0
0157	0
0158	0
0159	0
0160	0
0161	0
0162	0
0163	0
0164	0
0165	0
0166	0
0167	0
0168	0
0169	0
0170	0
0171	0
0172	0
0173	0
0174	0
0175	0
0176	0
0177	0
0178	0
0179	0
0180	0
0181	0
0182	0
0183	0
0184	0
0185	0
0186	0
0187	0
0188	0
0189	0
0190	0
0191	0
0192	0
0193	0
0194	0
0195	0
0196	0
0197	0
0198	0
0199	0
0200	0
0201	0
0202	0
0203	0
0204	0
0205	0
0206	0
0207	0
0208	0
0209	0
0210	0
0211	0
0212	0
0213	0
0214	0
0215	0
0216	0
0217	0
0218	0
0219	0
0220	0
0221	0
0222	0
0223	0
0224	0
0225	0
0226	0
0227	0
0228	0
0229	0
0230	0
0231	0
0232	0
0233	0
0234	0
0235	0
0236	0
0237	0
0238	0
0239	0
0240	0
0241	0
0242	0
0243	0
0244	0
0245	0
0246	0
0247	0
0248	0
0249	0
0250	0
0251	0
0252	0
0253	0
0254	0
0255	0
0256	0
0257	0
0258	0
0259	0
0260	0
0261	0
0262	0
0263	0
0264	0
0265	0
0266	0
0267	0
0268	0
0269	0
0270	0
0271	0
0272	0
0273	0
0274	0
0275	0
0276	0
0277	0
0278	0
0279	0
0280	0
0281	0
0282	0
0283	0
0284	0
0285	0
0286	0
0287	0
0288	0
0289	0
0290	0
0291	0
0292	0
0293	0
0294	0
0295	0
0296	0
0297	0
0298	0
0299	0
0300	0
0301	0
0302	0
0303	0
0304	0
0305	0
0306	0
0307	0
0308	0
0309	0
0310	0
0311	0
0312	0
0313	0
0314	0
0315	0
0316	0
0317	0
0318	0
0319	0
0320	0
0321	0
0322	0
0323	0
0324	0
0325	0
0326	0
0327	0
0328	0
0329	0
0330	0
0331	0
0332	0
0333	0
0334	0
0335	0
0336	0
0337	0
0338	0
0339	0
0340	0
0341	0
0342	0
0343	0
0344	0
0345	0
0346	0
0347	0
0348	0
0349	0
0350	0
0351	0
0352	0
0353	0
0354	0
0355	0
0356	0
0357	0
0358	0
0359	0
0360	0
0361	0
0362	0
0363	0
0364	0
0365	0
0366	0
0367	0
0368	0
0369	0
0370	0
0371	0
0372	0
0373	0
0374	0
0375	0
0376	0
0377	0
0378	0
0379	0
0380	0
0381	0
0382	0
0383	0
0384	0
0385	0
0386	0
0387	0
0388	0
0389	0
0390	0
0391	0
0392	0
0393	0
0394	0
0395	0
0396	0
0397	0
0398	0
0399	0
0400	0
0401	0
0402	0
0403	0
0404	0
0405	0
0406	0
0407	0
0408	0
0409	1
0410	1
0411	0
0412	1
0413	2
0414	3
0415	4
0416	5
0417	6
0418	7
0419	8
0420	9
0421	10
0422	11
0423	12
0424	13
0425	14
0426	15
0427	16
0428	17
0429	18
0430	19
0431	20
0432	21
0433	22
0434	23
0435	24
0436	25
0437	26
0438	27
0439	28
0440	29
0441	30
0442	31
0443	32
0444	0
0445	0
0446	0
0447	0
0448	0
0449	0
0450	0
0451	0
0452	0
0453	0
0454	0
0455	0
0456	0
0457	0
0458	0
0459	0
0460	0
0461	0
0462	0
0463	0
0464	0
0465	0
0466	0
0467	0
0468	0
0469	0
0470	0
0471	0
0472	0
0473	0
0474	0
0475	0
0476	0
0477	0
0478	0
0479	0
0480	0
0481	0
0482	0
0483	0
0484	0
0485	0
0486	0
0487	0
0488	0
0489	0
0490	0
0491	0
0492	0
0493	0
0494	0
0495	0
0496	0
0497	0
0498	0
0499	0
0500	0
0501	0
0502	0
0503	0
0504	0
0505	0
0506	0
0507	0
0508	0
0509	0
0510	0
0511	0
0512	0
0513	0
0514	0
0515	0
0516	0
0517	0
0518	0
0519	0
0520	0
0521	0
0522	0
0523	0
0524	0
0525	0
0526	0
0527	0
0528	0
0529	0
0530	0
0531	0
0532	0
0533	0
0534	0
0535	0
0536	0
0537	0
0538	0
0539	0
0540	0
0541	0
0542	0
0543	0
0544	0
0545	0
0546	0
0547	0
0548	0
0549	0
0550	0
0551	0
0552	0
0553	0
0554	0
0555	0
0556	0
0557	0
0558	0
0559	0
0560	0
0561	0
0562	0
0563	0
0564	0
0565	0
0566	0
0567	0
0568	0
0569	0
0570	0
0571	0
0572	0
0573	0
0574	0
0575	0
0576	0
0577	0
0578	0
0579	0
0580	0
0581	0
0582	0
0583	0
0584	0
0585	0
0586	0
0587	0
0588	0
0589	0
0590	0
0591	0
0592	0
0593	0
0594	0
0595	0
0596	0
0597	0
0598	0
0599	0
0600	0
0601	0
0602	0
0603	0
0604	0
0605	0
0606	0
0607	0
0608	0
0609	0
0610	0
0611	0
0612	0
0613	0
0614	0
0615	0
0616	0
0617	0
0618	0
0619	0
0620	0
0621	0
0622	0
0623	0
0624	0
0625	0
0626	0
0627	0
0628	0
0629	0
0630	0
0631	0
0632	0
0633	0
0634	0
0635	0
0636	0
0637	0
0638	0
0639	0
0640	0
0641	0
0642	0
0643	0
0644	0
0645	0
0646	0
0647	0
0648	0
0649	0
0650	0
0651	0
0652	0
0653	0
0654	0
0655	0
0656	0
0657	0
0658	0
0659	0
0660	0
0661	0
0662	0
0663	0
0664	0
0665	0
0666	0
0667	0
0668	0
0669	0
0670	0
0671	0
0672	0
0673	0
0674	0
0675	0
0676	0
0677	0
0678	0
0679	0
0680	0
0681	0
0682	0
0683	0
0684	0
0685	0
0686	0
0687	0
0688	0
0689	0
0690	0
0691	0
0692	0
0693	0
0694	0
0695	0
0696	0
0697	0
0698	0
0699	0
0700	0
0701	0
0702	0
0703	0
0704	0
0705	0
0706	0
0707	0
0708	0
0709	0
0710	0
0711	0
0712	0
0713	0
0714	0
0715	0
0716	0
0717	0
0718	0
0719	0
0720	0
0721	0
0722	0
0723	0
0724	0
0725	0
0726	0
0727	0
0728	0
0729	0
0730	0
0731	0
0732	0
0733	0
0734	0
0735	0
0736	0
0737	0
0738	0
0739	0
0740	0
0741	0
0742	0
0743	0
0744	0
0745	0
0746	0
0747	0
0748	0
0749	0
0750	0
0751	0
0752	0
0753	0
0754	0
0755	0
0756	0
0757	0
0758	0
0759	0
0760	0
0761	0
0762	0
0763	0
0764	0
0765	0
0766	0
0767	0
0768	0
0769	0
0770	0
0771	0
0772	0
0773	0
0774	0
0775	0
0776	0
0777	0
0778	0
0779	0
0780	0
0781	0
0782	0
0783	0
0784	0
0785	0
0786	0
0787	0
0788	0
0789	0
0790	0
0791	0
0792	0
0793	0
0794	0
0795	0
0796	0
0797	0
0798	0
0799	0
0800	0
0801	0
0802	0
0803	0
0804	0
0805	0
0806	0
0807	0
0808	0
0809	0
0810	0
0811	0
0812	0
0813	0
0814	0
0815	0
0816	0
0817	0
0818	0
0819	0
0820	0
0821	0
0822	0
0823	0
0824	0
0825	0
0826	0
0827	0
0828	0
0829	0
0830	0
0831	0
0832	0
0833	0
0834	0
0835	0
0836	0
0837	0
0838	0
0839	0
0840	0
0841	0
0842	0
0843	0
0844	0
0845	0
0846	0
0847	0
0848	0
0849	0
0850	0
0851	0
0852	0
0853	0
0854	0
0855	0
0856	0
0857	0
0858	0
0859	0
0860	0
0861	0
0862	0
0863	0
0864	0
0865	0
0866	0
0867	0
0868	0
0869	0
0870	0
0871	0
0872	0
0873	0
0874	0
0875	0
0876	0
0877	0
0878	0
0879	0
0880	0
0881	0
0882	0
0883	0
0884	0
0885	0
0886	0
0887	0
0888	0
0889	0
0890	0
0891	0
0892	0
0893	0
0894	0
0895	0
0896	0
0897	0
0898	0
0899	0
0900	0
0901	0
0902	0
0903	0
0904	0
0905	0
0906	0
0907	0
0908	0
0909	0
0910	0
0911	0
0912	0
0913	0
0914	0
0915	0
0916	0
0917	0
0918	0
0919	0
0920	0
0921	0
0922	0
0923	0
0924	0
0925	0
0926	0
0927	0
0928	0
0929	0
0930	0
0931	0
0932	0
0933	0
0934	0
0935	0
0936	0
0937	0
0938	0
0939	0
0940	0
0941	0
0942	0
0943	0
0944	0
0945	0
0946	0
0947	0
0948	0
0949	0
0950	0
0951	0
0952	0
0953	0
0954	0
0955	0
0956	0
0957	0
0958	0
0959	0
0960	0
0961	0
0962	0
0963	0
0964	0
0965	0
0966	0
0967	0
0968	0
0969	0
0970	0
0971	0
0972	0
0973	0
0974	0
0975	0
0976	0
0977	0
0978	0
0979	0
0980	0
0981	0
0982	0
0983	0
0984	0
0985	0
0986	0
0987	0
0988	0
0989	0
0990	0
0991	0
0992	0
0993	0
0994	0
0995	0
0996	0
0997	0
0998	0
0999	0
1000	0
END_PLC_INIT_D

PLC_INIT_DC
TOTALTIPS	100
0001	0
0002	0
0003	0
0004	0
0005	0
0006	0
0007	0
0008	0
0009	0
0010	0
0011	0
0012	0
0013	0
0014	0
0015	0
0016	0
0017	0
0018	0
0019	0
0020	0
0021	0
0022	0
0023	0
0024	0
0025	0
0026	0
0027	0
0028	0
0029	0
0030	0
0031	0
0032	0
0033	0
0034	0
0035	0
0036	0
0037	0
0038	0
0039	0
0040	0
0041	0
0042	0
0043	0
0044	0
0045	0
0046	0
0047	0
0048	0
0049	0
0050	0
0051	0
0052	0
0053	0
0054	0
0055	0
0056	0
0057	0
0058	0
0059	0
0060	0
0061	0
0062	0
0063	0
0064	0
0065	0
0066	0
0067	0
0068	0
0069	0
0070	0
0071	0
0072	0
0073	0
0074	0
0075	0
0076	0
0077	0
0078	0
0079	0
0080	0
0081	0
0082	0
0083	0
0084	0
0085	0
0086	0
0087	0
0088	0
0089	0
0090	0
0091	0
0092	0
0093	0
0094	0
0095	0
0096	0
0097	0
0098	0
0099	0
0100	0
END_PLC_INIT_DC

PLC_INIT_DT
TOTALTIPS	100
0001	0
0002	0
0003	0
0004	0
0005	0
0006	0
0007	0
0008	0
0009	0
0010	0
0011	0
0012	0
0013	0
0014	0
0015	10000
0016	3000
0017	500000
0018	0
0019	0
0020	100
0021	500
0022	500
0023	100
0024	500
0025	700
0026	10000
0027	50000
0028	50000
0029	50000
0030	10000
0031	10000
0032	200
0033	5000
0034	5000
0035	10000
0036	0
0037	0
0038	0
0039	0
0040	0
0041	0
0042	0
0043	0
0044	0
0045	0
0046	0
0047	0
0048	0
0049	0
0050	0
0051	0
0052	0
0053	0
0054	0
0055	0
0056	0
0057	0
0058	0
0059	0
0060	0
0061	0
0062	0
0063	0
0064	0
0065	0
0066	0
0067	0
0068	0
0069	0
0070	0
0071	0
0072	0
0073	0
0074	0
0075	0
0076	0
0077	0
0078	0
0079	0
0080	0
0081	0
0082	0
0083	0
0084	0
0085	0
0086	0
0087	0
0088	0
0089	0
0090	0
0091	0
0092	0
0093	0
0094	0
0095	0
0096	0
0097	0
0098	0
0099	0
0100	0
END_PLC_INIT_DT

INITDATA_DC
TOTALTIPS	100
0001	0	7FFFFFFF	0	
0002	0	7FFFFFFF	0	
0003	0	7FFFFFFF	0	
0004	0	7FFFFFFF	0	
0005	0	7FFFFFFF	0	
0006	0	7FFFFFFF	0	
0007	0	7FFFFFFF	0	
0008	0	7FFFFFFF	0	
0009	0	7FFFFFFF	0	
0010	0	7FFFFFFF	0	
0011	0	7FFFFFFF	0	
0012	0	7FFFFFFF	0	
0013	0	7FFFFFFF	0	
0014	0	7FFFFFFF	0	
0015	0	7FFFFFFF	0	
0016	0	7FFFFFFF	0	
0017	0	7FFFFFFF	0	
0018	0	7FFFFFFF	0	
0019	0	7FFFFFFF	0	
0020	0	7FFFFFFF	0	
0021	0	7FFFFFFF	0	
0022	0	7FFFFFFF	0	
0023	0	7FFFFFFF	0	
0024	0	7FFFFFFF	0	
0025	0	7FFFFFFF	0	
0026	0	7FFFFFFF	0	
0027	0	7FFFFFFF	0	
0028	0	7FFFFFFF	0	
0029	0	7FFFFFFF	0	
0030	0	7FFFFFFF	0	
0031	0	7FFFFFFF	0	
0032	0	7FFFFFFF	0	
0033	0	7FFFFFFF	0	
0034	0	7FFFFFFF	0	
0035	0	7FFFFFFF	0	
0036	0	7FFFFFFF	0	
0037	0	7FFFFFFF	0	
0038	0	7FFFFFFF	0	
0039	0	7FFFFFFF	0	
0040	0	7FFFFFFF	0	
0041	0	7FFFFFFF	0	
0042	0	7FFFFFFF	0	
0043	0	7FFFFFFF	0	
0044	0	7FFFFFFF	0	
0045	0	7FFFFFFF	0	
0046	0	7FFFFFFF	0	
0047	0	7FFFFFFF	0	
0048	0	7FFFFFFF	0	
0049	0	7FFFFFFF	0	
0050	0	7FFFFFFF	0	
0051	0	7FFFFFFF	0	
0052	0	7FFFFFFF	0	
0053	0	7FFFFFFF	0	
0054	0	7FFFFFFF	0	
0055	0	7FFFFFFF	0	
0056	0	7FFFFFFF	0	
0057	0	7FFFFFFF	0	
0058	0	7FFFFFFF	0	
0059	0	7FFFFFFF	0	
0060	0	7FFFFFFF	0	
0061	0	7FFFFFFF	0	
0062	0	7FFFFFFF	0	
0063	0	7FFFFFFF	0	
0064	0	7FFFFFFF	0	
0065	0	7FFFFFFF	0	
0066	0	7FFFFFFF	0	
0067	0	7FFFFFFF	0	
0068	0	7FFFFFFF	0	
0069	0	7FFFFFFF	0	
0070	0	7FFFFFFF	0	
0071	0	7FFFFFFF	0	
0072	0	7FFFFFFF	0	
0073	0	7FFFFFFF	0	
0074	0	7FFFFFFF	0	
0075	0	7FFFFFFF	0	
0076	0	7FFFFFFF	0	
0077	0	7FFFFFFF	0	
0078	0	7FFFFFFF	0	
0079	0	7FFFFFFF	0	
0080	0	7FFFFFFF	0	
0081	0	7FFFFFFF	0	
0082	0	7FFFFFFF	0	
0083	0	7FFFFFFF	0	
0084	0	7FFFFFFF	0	
0085	0	7FFFFFFF	0	
0086	0	7FFFFFFF	0	
0087	0	7FFFFFFF	0	
0088	0	7FFFFFFF	0	
0089	0	7FFFFFFF	0	
0090	0	7FFFFFFF	0	
0091	0	7FFFFFFF	0	
0092	0	7FFFFFFF	0	
0093	0	7FFFFFFF	0	
0094	0	7FFFFFFF	0	
0095	0	7FFFFFFF	0	
0096	0	7FFFFFFF	0	
0097	0	7FFFFFFF	0	
0098	0	7FFFFFFF	0	
0099	0	7FFFFFFF	0	
0100	0	7FFFFFFF	0	
END_INITDATA_DC

INITDATA_DT
TOTALTIPS	100
0001	0	7FFFFFFF	0	
0002	0	7FFFFFFF	0	
0003	0	7FFFFFFF	0	
0004	0	7FFFFFFF	0	
0005	0	7FFFFFFF	0	
0006	0	7FFFFFFF	0	
0007	0	7FFFFFFF	0	
0008	0	7FFFFFFF	0	
0009	0	7FFFFFFF	0	
0010	0	7FFFFFFF	0	
0011	0	7FFFFFFF	0	
0012	0	7FFFFFFF	0	
0013	0	7FFFFFFF	0	
0014	0	7FFFFFFF	0	
0015	2710	7FFFFFFF	0	
0016	BB8	7FFFFFFF	0	
0017	7A120	7FFFFFFF	0	
0018	0	7FFFFFFF	0	
0019	0	7FFFFFFF	0	
0020	64	7FFFFFFF	0	
0021	1F4	7FFFFFFF	0	
0022	1F4	7FFFFFFF	0	
0023	64	7FFFFFFF	0	
0024	1F4	7FFFFFFF	0	
0025	2BC	7FFFFFFF	0	
0026	2710	7FFFFFFF	0	
0027	C350	7FFFFFFF	0	
0028	C350	7FFFFFFF	0	
0029	C350	7FFFFFFF	0	
0030	2710	7FFFFFFF	0	
0031	2710	7FFFFFFF	0	
0032	C8	FFF	0	
0033	1388	7FFFFFFF	0	
0034	1388	7FFFFFFF	0	
0035	2710	7FFFFFFF	0	
0036	0	7FFFFFFF	0	
0037	0	7FFFFFFF	0	
0038	0	7FFFFFFF	0	
0039	0	7FFFFFFF	0	
0040	0	7FFFFFFF	0	
0041	0	7FFFFFFF	0	
0042	0	7FFFFFFF	0	
0043	0	7FFFFFFF	0	
0044	0	7FFFFFFF	0	
0045	0	7FFFFFFF	0	
0046	0	7FFFFFFF	0	
0047	0	7FFFFFFF	0	
0048	0	7FFFFFFF	0	
0049	0	7FFFFFFF	0	
0050	0	7FFFFFFF	0	
0051	0	7FFFFFFF	0	
0052	0	7FFFFFFF	0	
0053	0	7FFFFFFF	0	
0054	0	7FFFFFFF	0	
0055	0	7FFFFFFF	0	
0056	0	7FFFFFFF	0	
0057	0	7FFFFFFF	0	
0058	0	7FFFFFFF	0	
0059	0	7FFFFFFF	0	
0060	0	7FFFFFFF	0	
0061	0	7FFFFFFF	0	
0062	0	7FFFFFFF	0	
0063	0	7FFFFFFF	0	
0064	0	7FFFFFFF	0	
0065	0	7FFFFFFF	0	
0066	0	7FFFFFFF	0	
0067	0	7FFFFFFF	0	
0068	0	7FFFFFFF	0	
0069	0	7FFFFFFF	0	
0070	0	7FFFFFFF	0	
0071	0	7FFFFFFF	0	
0072	0	7FFFFFFF	0	
0073	0	7FFFFFFF	0	
0074	0	7FFFFFFF	0	
0075	0	7FFFFFFF	0	
0076	0	7FFFFFFF	0	
0077	0	7FFFFFFF	0	
0078	0	7FFFFFFF	0	
0079	0	7FFFFFFF	0	
0080	0	7FFFFFFF	0	
0081	0	7FFFFFFF	0	
0082	0	7FFFFFFF	0	
0083	0	7FFFFFFF	0	
0084	0	7FFFFFFF	0	
0085	0	7FFFFFFF	0	
0086	0	7FFFFFFF	0	
0087	0	7FFFFFFF	0	
0088	0	7FFFFFFF	0	
0089	0	7FFFFFFF	0	
0090	0	7FFFFFFF	0	
0091	0	7FFFFFFF	0	
0092	0	7FFFFFFF	0	
0093	0	7FFFFFFF	0	
0094	0	7FFFFFFF	0	
0095	0	7FFFFFFF	0	
0096	0	7FFFFFFF	0	
0097	0	7FFFFFFF	0	
0098	0	7FFFFFFF	0	
0099	0	7FFFFFFF	0	
0100	0	7FFFFFFF	0	
END_INITDATA_DT

INITDATA_K
TOTALTIPS	40
0001	0	
0002	0	
0003	0	
0004	0	
0005	0	
0006	0	
0007	0	
0008	0	
0009	0	
0010	0	
0011	0	
0012	5	
0013	0	
0014	0	
0015	0	
0016	0	
0017	0	
0018	0	
0019	0	
0020	0	
0021	0	
0022	0	
0023	0	
0024	0	
0025	0	
0026	0	
0027	0	
0028	0	
0029	0	
0030	0	
0031	0	
0032	0	
0033	0	
0034	0	
0035	0	
0036	0	
0037	0	
0038	0	
0039	0	
0040	0	
END_INITDATA_K

PLC_SYMBOL
TOTALTIPS	201
0001	D0408	Target No Pocket	
0002	D0409	The current number of pocket	
0003	D0410	The current number of pockets on the spindle	
0004	D0411	The tool of number under the pocket number 1	
0005	D0412	The tool of number under the pocket number 2	
0006	D0413	The tool of number under the pocket number 3	
0007	D0414	The tool of number under the pocket number 4	
0008	D0415	The tool of number under the pocket number 5	
0009	D0416	The tool of number under the pocket number 6	
0010	D0417	The tool of number under the pocket number 7	
0011	D0418	The tool of number under the pocket number 8	
0012	D0419	The tool of number under the pocket number 9	
0013	D0420	The tool of number under the pocket number 10	
0014	D0421	The tool of number under the pocket number 11	
0015	D0422	The tool of number under the pocket number 12	
0016	D0423	The tool of number under the pocket number 13	
0017	D0424	The tool of number under the pocket number 14	
0018	D0425	The tool of number under the pocket number 15	
0019	D0426	The tool of number under the pocket number 16	
0020	D0427	The tool of number under the pocket number 17	
0021	D0428	The tool of number under the pocket number 18	
0022	D0429	The tool of number under the pocket number 19	
0023	D0430	The tool of number under the pocket number 20	
0024	D0431	The tool of number under the pocket number 21	
0025	D0432	The tool of number under the pocket number 22	
0026	D0433	The tool of number under the pocket number 23	
0027	D0434	The tool of number under the pocket number 24	
0028	D0435	The tool of number under the pocket number 25	
0029	D0436	The tool of number under the pocket number 26	
0030	D0437	The tool of number under the pocket number 27	
0031	D0438	The tool of number under the pocket number 28	
0032	D0439	The tool of number under the pocket number 29	
0033	D0440	The tool of number under the pocket number 30	
0034	D0441	The tool of number under the pocket number 31	
0035	D0442	The tool of number under the pocket number 32	
0036	DT0014	time of spindle orientation	
0037	DT0015	time of checking VP(X5.0)after M29 is executed	
0038	DT0016	time of auto lubrication cancel	
0039	DT0017	0£ºnot auto lubrication,>0£ºauto lubrication	
0040	DT0018	not auto lubr..0£ºalternative lubrication,>0£ºschedular lubrication	
0041	DT0019	time of S execution	
0042	DT0020	time of T execution	
0043	DT0021	time of M execution	
0044	DT0022	time from spinlde stop to output brake	
0045	DT0023	time of spindle output brake	
0046	DT0024	delay tiem of spindle changing gear	
0047	DT0025	Discal tool M instruction execution time	
0048	DT0026	Armless type ATC M instruction execution time	
0049	DT0027	Processing time for tool change arm	
0050	DT0028	Tool time for pre-cutter	
0051	DT0029	Executive M14, detection VP (X5.1) of the time	
0052	DT0030	Elastic the spindle tool  delay time	
0053	DT0031	Spindle speed automatic shift	
0054	DT0032	Automatic gear shift off the original time	
0055	DT0033	Automatic transmission in place after the end of time delay	
0056	DT0034	Automatic shift detection time	
0057	K0000	No Recompose	
0058	K0001	No Recompose	
0059	K0002	No Recompose	
0060	K0003	No Recompose	
0061	K0004	No Recompose	
0062	K0005	No Recompose	
0063	K0006	No Recompose	
0064	K0007	No Recompose	
0065	K0008	No Recompose	
0066	K0009	No Recompose	
0067	K0010	*** *** *** JSPD OVRI OUTR RSJG RESB	
0068	K0010.0	$RESB$1/0:with reset,Cursor return/not in AUTO mode	
0069	K0010.1	$RSJG$1/0:with reset ,spindle¡¢coolant¡¢lubrication retain/cancel	
0070	K0010.2	$OUTR$1/0:as restart key,"DATA OUTPUT" key is valdi /invalid,	
0071	K0010.3	$OVRI$1/0:feed rate is 100%/can be adjusted	
0072	K0010.4	$JSPD$1/0:spindle jog is valid in all mode/JOG¡¢MPG¡¢REF mode	
0073	K0010.5	reserved	
0074	K0010.6	reserved	
0075	K0010.7	reserved	
0076	K0011	HALT1 HALT2 ELDH *** TDLC REFP APCH TTCM	
0077	K0011.0	$TTCM$ATC arm is not in place 1:Locked to the signal 0: Not locked to the signal	
0078	K0011.1	$APCH$1/0:Does not detect / detect cylinder pressure is too low	
0079	K0011.2	$REFP$1/0:Exchange before testing tool / does not detect the reference point	
0080	K0011.3	$TDLC$1/0:Exchange of tool, the detection / non-detection tool knife Elastic state	
0081	K0011.4	$HTCY$1/0:Exchange before testing tool / does not detect the third reference point	
0082	K0011.5	$ELDH$1/0:Loosen the tool to clamp the tool function valid / invalid	
0083	K0011.6	$HILT2$HILT1¡¢HALT2£º10£ºBT40 discal tool valid 01£ºArmless type ATC valid	
0084	K0011.7	$HILT1$HILT1¡¢HALT2£º00£ºtool function invalid 11£ºtool function invalid	
0085	K0012	SPCD EMS *** *** *** *** *** SPSE	
0086	K0012.0	$SPSE$1/0:Spindle automatic transmission signal to keep / not keep	
0087	K0012.6	$EMS$1/0£ºMultiple spindle function valid / invalid	
0088	K0012.7	$SPCD$1/0:Spindle automatic shift function is valid / invalid	
0089	K0013	NMAX *** *** *** *** *** *** ***	
0090	K0013.0	reserved	
0091	K0013.1	reserved	
0092	K0013.7	$NMAX$1/0:Hand-wheel single-step mode, ¡Á1000 rate key invalid / valid	
0093	K0015	LTEN  LUSE  *** *** *** *** *** LTHL	
0094	K0015.0	$LTHL$1/0:X\Y\Zaxis overtravel limi low/high level alarm	
0095	K0015.1	reserved	
0096	K0015.2	reserved	
0097	K0015.3	reserved	
0098	K0015.4	reserved	
0099	K0015.5	reserved	
0100	K0015.6	$LUSE$1/0:signal of checking lubrication oil press low is high/low,when alarm occurs	
0101	K0015.7	$LTEN$1/0:check/no check X\Y\Z external overtravel limit signal	
0102	T0000	count time of executing S code	
0103	X0000	TVCH THCH ESP TCOT DECX  TPCH  SP TDEC	
0104	X0000.0	$TDEC$tool to zero signal	
0105	X0000.1	$SP$external SP signal	
0106	X0000.2	$TPCH$cylinder pressure check	
0107	X0000.3	$DECX$X axis deceleration signal	
0108	X0000.4	$TCOT$take count of tool	
0109	X0000.5	$ESP$External urgent stop signal	
0110	X0000.6	$THCH$Pocket level in place/Cutter back in place	
0111	X0000.7	$TVCH$Vertical pocket in place/Cutter in place ahead	
0112	X0001	TRCH GECK1 JOGT  ST DECZ THZP  THGT THSP	
0113	X0001.0	$THSP$ATC arm stop checking(discal tool)	
0114	X0001.1	$THGT$ATC arm to seize the tool checks(discal tool)	
0115	X0001.2	$THZP$ATC arm back the origin check(discal tool)	
0116	X0001.3	$DECZ$Z axis deceleration signal	
0117	X0001.4	$ST$External cycle start signal	
0118	X0001.5	$JOGT$External Elastic tool spindle input signal	
0119	X0001.6	$GECK1$Detection of the first tranche of the spindle in place	
0120	X0001.7	$TRCH$Loosen the spindle position check tool	
0121	X0002	LTXN_LUBC GECK2  DEC5 DEC4 DECY TTOV THOV TGGH	
0122	X0002.0	$TGGH$check the clamping tool	
0123	X0002.1	$THOV$ATC arm motor overload(discal tool)	
0124	X0002.2	$TTOV$tool motor overload(discal tool/armless tool)	
0125	X0002.3	$DECY$Y axis deceleration signal	
0126	X0002.4	$DEC4$4th axis deceleration signal	
0127	X0002.5	$DEC5$5th axis deceleration signal	
0128	X0002.6	$GECK2$Detection of the second tranche of the spindle in place	
0129	X0002.7	$LTXN_LUBC$X- overtravel limit input/lubrication oil press check	
0130	X0003	LTZP LTZN SKIP GECK4 GECK3 LTYP LTYN LTXP	
0131	X0003.0	$LTXP$X+ overtravel limit input	
0132	X0003.1	$LTYN$Y- overtravel limit input	
0133	X0003.2	$LTYP$Y+ overtravel limit input	
0134	X0003.3	$GECK3$Detection of the third tranche of the spindle in place	
0135	X0003.4	$GECK4$Detection of the fourth tranche of the spindle in place	
0136	X0003.5	$SKIP$G31 skip signal	
0137	X0003.6	$LTZN$Z- overtravel limit input	
0138	X0003.7	$LTZP$Z+ overtravel limit input	
0139	X0005	*** *** *** *** SPAL COIN *** VP0	
0140	X0005.0	$VP0$indicator of spindle V/P	
0141	X0005.1	reserved	
0142	X0005.2	$COIN$coin signal	
0143	X0005.3	$SPAL$the spindle alam signal	
0144	X0005.4	reserved	
0145	X0005.5	reserved	
0146	X0005.6	reserved	
0147	X0005.7	reserved	
0148	X0006	*** *** EMP2 EMP1 EMP0 EHDZ EHDY EHDX	
0149	X0006.0	$EHDX$external MPG X choosed	
0150	X0006.1	$EHDY$external MPG Y choosed	
0151	X0006.2	$EHDZ$external MPG Z choosed	
0152	X0006.3	$EMP0$external X1 rate	
0153	X0006.4	$EMP1$external X10 rate	
0154	X0006.5	$EMP2$external X100 rate	
0155	X0006.6	reserved	
0156	X0006.7	reserved	
0157	Y0000	SPZD *** SSTP SFR SRV *** LUBR COOL	
0158	Y0000.0	$COOL$Cooling signal	
0159	Y0000.1	$LUBR$Lubricating output signal	
0160	Y0000.2	reserved	
0161	Y0000.3	SFR,Spindle CCW signal	
0162	Y0000.4	SRV,Spindle CW signal	
0163	Y0000.5	$SSTP$Spindle stop signal	
0164	Y0000.6	reserved	
0165	Y0000.7	$SPZD$Spindle braking signal	
0166	Y0001	TCCW TCW TVER THOR  GEAR4 GEAR3 GEAR2 GEAR1	
0167	Y0001.0	$GEAR1$Spindle mechanical gear signal 1	
0168	Y0001.1	$GEAR2$Spindle mechanical gear signal 2	
0169	Y0001.2	$GEAR3$Spindle mechanical gear signal 3	
0170	Y0001.3	$GEAR4$Spindle mechanical gear signal 4	
0171	Y0001.4	$THOR$Vertical pocket/Cutter Forward	
0172	Y0001.5	$TVER$Pocket level/Cutter back	
0173	Y0001.6	$TCW$tool motor cw	
0174	Y0001.7	$TCCW$tool motor ccw	
0175	Y0002	ALTO *** *** CLPR CLPG CLPY THOT TROT	
0176	Y0002.0	$TROT$the clamping/releasing tool signal	
0177	Y0002.1	$THOT$ATC arm  motor output signal	
0178	Y0002.2	$CLPY$CLPY,Yellow light	
0179	Y0002.3	$CLPG$CLPG,Green light	
0180	Y0002.4	$CLPR$CLPR,Red light	
0181	Y0002.5	reserved	
0182	Y0002.6	reserved	
0183	Y0002.7	$ALTO$ALT. output signal	
0184	Y0003	*** *** SPZD2 SRV2 SFR2 *** *** STAO	
0185	Y0003.0	$STAO$the spindle directional signal	
0186	Y0003.1	reserved	
0187	Y0003.2	reserved	
0188	Y0003.3	$SFR2$the second spindle cw	
0189	Y0003.4	$SRV2$the second spindle ccw	
0190	Y0003.5	$SPZD2$the second soindle braking signal	
0191	Y0003.6	reserved	
0192	Y0003.7	reserved	
0193	Y0005	*** *** *** *** SFR SRV TAP VP	
0194	Y0005.0	$VP$spindle V/P switch	
0195	Y0005.1	$TAP$TAP singal	
0196	Y0005.2	$SRV$the first spindle ccw	
0197	Y0005.3	$SFR$the first spindle cw	
0198	Y0005.4	reserved	
0199	Y0005.5	reserved	
0200	Y0005.6	reserved	
0201	Y0005.7	reserved	
END_PLC_SYMBOL

NETWORK_COMMENT
TOTALTIPS	0
END_NETWORK_COMMENT

NETWORK_COMMENT_ADDSECTION

BLOCK_INF
Level1
¹ãÖÝÊý¿Ø
V2.0-08.05.20
GSK980MDa±ê×¼ÌÝÐÎÍ¼
BLOCK_INF_END

BLOCK_INF
Level2



BLOCK_INF_END

COMMENT_START
K10.0--1:Cursor returns in auto mode
COMMENT_END

COMMENT_START
R335.0---Sign of AUTO¡¢MDI¡¢DNC mode.
COMMENT_END

COMMENT_START
R335.7:F0¡¢25%¡¢50%¡¢100% key can be used to adjust rapid rate in AUTO¡¢MDI¡¢DNC¡¢JOG RAPID mode¡£
COMMENT_END

COMMENT_START
R335.1:sign of EDIT¡¢MPG/STEP¡¢JOG¡¢REF mode
COMMENT_END

COMMENT_START
R17.0:sign of AUTO¡¢MDI¡¢DNC¡¢EDIT mode
COMMENT_END

COMMENT_START
R138.0£ºsign of MPG¡¢STEP mode
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Mode will be retained when power on
COMMENT_END

COMMENT_START
single block¡¢skip block¡¢machine lock¡¢mst lock¡¢dry run fail when power on

COMMENT_END

COMMENT_START
R135.4£ºmode key is pressed
COMMENT_END

COMMENT_START
X19.3£ºDNC mode key
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Y23.3£ºindicator of MPG/STEP mode
COMMENT_END

COMMENT_START
Y23.2£ºindicator of JOG mode
COMMENT_END

COMMENT_START
Y23.5£ºindicator of MDI mode
COMMENT_END

COMMENT_START
Y23.6£ºindicator of AUTO mode
COMMENT_END

COMMENT_START
Y23.7£ºindicator of EDIT mode
COMMENT_END

COMMENT_START
Y23.4£ºindicator of REF mode
COMMENT_END

COMMENT_START
Y18.2£ºindicator of DNC mode
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
K15.7:1--¼ì²âXYZÍâ½Ó³¬³ÌÐÅºÅ
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X0.5£ºexternal ESP signal,if bit3 of bit parameter 17 is 1,the signal is invalid
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X1.4£ºrestart signal,if bit6 of bit parameter17 is 1,the signal is invalid
COMMENT_END

COMMENT_START
X0.1£ºexternal pause signal,If bit5 of bit parameter 17 is 1,the signal is invalid.
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
K10.2£ºif this signal is 1,the key"DATA Output" of panel can be used as restart key.

COMMENT_END

COMMENT_START
X23.0£ºrestart key of panel
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X22.7£ºpause key of panel
COMMENT_END

COMMENT_START
Y21.0£ºindicator of panel pause key .

COMMENT_END

COMMENT_START
Y20.0£ºindicator of panel restart key .

COMMENT_END

COMMENT_START
bit0 of bit parameter020(F214.0)£ºX direction define
COMMENT_END

COMMENT_START
bit1 of bit parameter020(F214.1)£ºY direction define
COMMENT_END

COMMENT_START
bit2 of bit parameter020(F214.2):Z direction define
COMMENT_END

COMMENT_START
bit3 of bit parameter020(F214.3)£º4th axis direction define
COMMENT_END

COMMENT_START
bit4 of bit parameter020(F214.4)£º5th axis direction define.
COMMENT_END

COMMENT_START
Y22.7:indicator of X ref
COMMENT_END

COMMENT_START
Y22.5£ºindicator of Y ref
COMMENT_END

COMMENT_START
Y22.6£ºindicator of Z ref
COMMENT_END

COMMENT_START
Y22.4£ºindicator of 4th ref
COMMENT_END

COMMENT_START
Y21.2:indicator of 5th ref
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X ref:+ move
COMMENT_END

COMMENT_START
X ref:- move
COMMENT_END

COMMENT_START
Y ref:+ move
COMMENT_END

COMMENT_START
Y ref:- move
COMMENT_END

COMMENT_START
Z ref:+ move
COMMENT_END

COMMENT_START
Z ref:- move
COMMENT_END

COMMENT_START
X:+ move
COMMENT_END

COMMENT_START
X:- move
COMMENT_END

COMMENT_START
Y:+ move
COMMENT_END

COMMENT_START
Y:- move
COMMENT_END

COMMENT_START
Z:+ move
COMMENT_END

COMMENT_START
Z:- move
COMMENT_END

COMMENT_START
4th :move subprogram

COMMENT_END

COMMENT_START
5th:move subprogram
COMMENT_END

COMMENT_START
P210£ºadjust feed rate in AUTO¡¢MDI¡¢DNC¡¢EDIT mode

COMMENT_END

COMMENT_START
P213:adjust feed rate in REF¡¢MPG¡¢STEP¡¢JOG mode
COMMENT_END

COMMENT_START
M8£½R4.0,    M10=R4.2,  M14=R4.6     M15=R4.7      M29--R5.0     M19---R22.5
COMMENT_END

COMMENT_START
R4.0£ºM8  R4.1(R119.0)£ºM9
COMMENT_END

COMMENT_START
R4.2£ºM10   R4.3(R119.1)£ºM11
COMMENT_END

COMMENT_START
X21.4£ºcoolant key
COMMENT_END

COMMENT_START
Y0.0£ºcoolant output    Y23.0£ºindicator of coolant output

COMMENT_END

COMMENT_START
R4.2£ºM10£¬reserved  R119.1£ºM11 reserved
COMMENT_END

COMMENT_START
Y1.1£ºoutput of M10/M11
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
R32.0£ºM32   R32.1(R119.2)£ºM33
COMMENT_END

COMMENT_START
DT17=0£ºnot auto lubrication
        >0£ºauto lubrication ,DT17:time of auto lubrication,DT16:time of cancelling output
DT18=0£ºnot auto lubrication ,alternative lubrication,
        >0£ºnot auto lubrication,schedular lubrication
COMMENT_END

COMMENT_START
output of alternative lubrication
COMMENT_END

COMMENT_START
output of schedular lubrication
COMMENT_END

COMMENT_START
output of auto lubrication
COMMENT_END

COMMENT_START
Y0.1£ºoutput signal of lubrication  Y20.7£ºpanel indicator of lubrication
COMMENT_END

COMMENT_START
R22.5--Ö÷ÖáËÙ¶È·½Ê½ÏÂµÄ×¼Í£             Y3.0--Ö÷Öá¶¨ÏòÆô¶¯ÐÅºÅ      Y21.3----Ö÷Öá×¼Í£µÆ
DT14---Ö÷Öá×¼Í£Ê±¼ä           X25.7---Ö÷Öá×¼Í£¼ü         X5.2---Ö÷Öá¶¨ÏòÍê³É
COMMENT_END

COMMENT_START
A0.4£ºÖ÷Öá×¼Í£Ê±¼ä¹ý³¤±¨¾¯
COMMENT_END

COMMENT_START
rigid tap process

COMMENT_END

COMMENT_START
R133.3£ºM3      R133.4£ºM4       R133.5(R143.5)£ºM5
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
when it is rotary,if the direction is changed in MDI mode,alarm A0.3 occurs:M03¡¢M04 error
COMMENT_END

COMMENT_START
X21.5£ºspindle stop key
COMMENT_END

COMMENT_START
X21.3£ºspindle cw key

COMMENT_END

COMMENT_START
X21.7£ºspindle ccw key
COMMENT_END

COMMENT_START
X25.5£ºspindle jog  key
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
sindle cw
COMMENT_END

COMMENT_START
Y21.1£ºindicator of spindle jog
COMMENT_END

COMMENT_START
Y0.4£ºspindle ccw output   Y19.1£ºindicator of sindle ccw output   F65.1£ºsign of rigid tap ccw
COMMENT_END

COMMENT_START
Y19.1£ºindicator of sindle ccw output   F65.1£ºsign of rigid tap ccw
COMMENT_END

COMMENT_START
spindle ccw
COMMENT_END

COMMENT_START
Y0.3£ºspindle cw output   Y23.1£ºindicator of sindle cw output   F65.0£ºsign of rigid tap cw
COMMENT_END

COMMENT_START
Y23.1£ºindicator of sindle cw output    F65.1£ºsign of rigid tap ccw
COMMENT_END

COMMENT_START
Y0.5:output signal of spindle stop  Y18.0:indicator of spindle stop
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
R307.0£ºthe sign that spindle is rotary
COMMENT_END

COMMENT_START
if spindle will be stopped,brake will be valid.
COMMENT_END

COMMENT_START
P307£ºspindle brake subprogram
COMMENT_END

COMMENT_START
Ë«Ö÷Öá¹¦ÄÜ
COMMENT_END

COMMENT_START
Ö÷Öá×Ô¶¯»»µ²¹¦ÄÜ
COMMENT_END

COMMENT_START
ÕûÀíµ¶ÅÌºó,×Ô¶¯¸üÐÂ¸üÐÂC22¡¢C23
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
½«µ¶¾ßÊý¸³Öµ¸øDC1

COMMENT_END

COMMENT_START
P30£ºBT50/40Ô²ÅÌÐÍµ¶¿â´¦Àí
COMMENT_END

COMMENT_START
P40£º¶·óÒÊ½µ¶¿â
COMMENT_END

COMMENT_START
Ö÷ÖáËÉ½ôµ¶
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
finished singal of M3¡¢4¡¢5¡¢8¡¢9¡¢10¡¢11¡¢32¡¢33¡¢29     DT21£ºtime of M execution
COMMENT_END

COMMENT_START
F9.4£ºM30   F9.5£ºM02   F9.6£ºM01   F9.7£ºM00
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
G4.3£ºfinished signal of auxiliary functionºÅ
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
K10.3-1:feed rate is 100%,
      0:feed rate can be adjusted
COMMENT_END

COMMENT_START
memory is open
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
R50.4--M54
R50.5--M55
R60.5--M65
R60.6--M66
R61.0--M68
R61.1--M69
R61.2--M70
R40.0--M19
R50.6--M56
R50.7--M57
          ----->R61.7

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
A0.0£ºillegal M code
COMMENT_END

COMMENT_START
P0£ºcolor lamp process subprogram
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
P1£ºsubprogram of choosing handwheel axis and adjusting mpg/step rate.
COMMENT_END

COMMENT_START
P2£ºsubprogram of adjusting rapid rate
COMMENT_END

COMMENT_START
turn off spindle rate light
COMMENT_END

COMMENT_START
P3£ºsubprogram of adjusting spindle rate
COMMENT_END

COMMENT_START
Ö÷ÖáÇÐ»»Îª¿ª¹ØÁ¿¿ØÖÆµÄÊ±ºò¹ØÖ÷Öá±¶ÂÊµÆ
COMMENT_END

COMMENT_START
turn off spindle rate light
COMMENT_END

COMMENT_START
P5£ºsubprogram of rapid move key
COMMENT_END

BLOCK_INF
sub0


color lamp process subprogram
BLOCK_INF_END

COMMENT_START
Y0.2£ºY0.2£ºyellow lamp
COMMENT_END

COMMENT_START
Y0.1£ºY0.1£ºgreen lamp
COMMENT_END

COMMENT_START
Y0.0£ºY0.0£ºred lamp
COMMENT_END

BLOCK_INF
sub1


subprogram of choosing handwheel axis and adjusting mpg/step rate.
BLOCK_INF_END

COMMENT_START
X19.4:X1(0.001) rate of MPG/STEP     X6.3:external X1 rate signal
COMMENT_END

COMMENT_START
X19.5:X10(0.010) rate of MPG/STEP     X6.4:external X10 rate signal
COMMENT_END

COMMENT_START
X19.6:X100(0.100) rate of MPG/STEP   X6.5:external X100 rate signal
COMMENT_END

COMMENT_START
X19.7:X1000(1.000) rate of MPG/STEP
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Y19.7£ºindicator of X1(0.001) rate of MPG/STEP
COMMENT_END

COMMENT_START
Y19.6£ºindicator of X10(0.010) rate of MPG/STEP
COMMENT_END

COMMENT_START
Y19.5£ºindicator of X100(0.100) rate of MPG/STEP
COMMENT_END

COMMENT_START
Y21.5£ºindicator of X1000(1.000) rate of MGP/STEP
COMMENT_END

COMMENT_START
X21.0:Y axis choosed in panle  X6.1£ºexternal signal of Y axis choosed
COMMENT_END

COMMENT_START
X20.3:Z axis choosed in panle  X6.2£ºexternal signal of Z axis choosed
COMMENT_END

COMMENT_START
X20.5:X axis choosed in panle  X6.0£ºexternal signal of X axis choosed
COMMENT_END

COMMENT_START
4th axis choosed
COMMENT_END

COMMENT_START
5th axis choosed
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
indicator of X handwheel
COMMENT_END

COMMENT_START
indicator of Y handwheel
COMMENT_END

COMMENT_START
indicator of Z handwheel
COMMENT_END

COMMENT_START
indicator of 4TH handwheel

COMMENT_END

COMMENT_START
indicator of 5TH handwheel
COMMENT_END

BLOCK_INF
sub2


subprogram of adjusting rapid rate
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Y20.2£ºmin.rapid rate(F0)

COMMENT_END

COMMENT_START
Y19.7£ºrapid rate (F0)
COMMENT_END

COMMENT_START
Y19.5£ºrapid rate:50%
COMMENT_END

COMMENT_START
Y19.6£ºrapid rate :25%
COMMENT_END

COMMENT_START
Y20.5£ºmax.rapid rate(100%)
COMMENT_END

COMMENT_START
Y21.5£ºrapid rate:100%
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
R3.0:max. rapid rate

COMMENT_END

COMMENT_START
R3.1£ºmin.rapid rate
COMMENT_END

COMMENT_START
X22.5£ºrapid rate key:-
COMMENT_END

COMMENT_START
X22.2£ºrapid rate key:+
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X19.4£ºrapid rate key:F0
COMMENT_END

COMMENT_START
X19.5£ºrapid rate key:25%
COMMENT_END

COMMENT_START
X19.6£ºrapid rate key:50%
COMMENT_END

COMMENT_START
X19.7£ºrapid rate key:100%
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub3


subprogram of adjusting spindle rate
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub4


subprogram of auxiliary function
BLOCK_INF_END

COMMENT_START
X19.1:auxiliary lock key Y18.4£ºindicator of auxiliary lock
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X19.0£ºmachine lock  Y18.5£ºindicator of machine lock
machine lock is valid in all mode
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X19.2£ºdry run key  Y18.3£ºindicator of dry run
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X18.6£ºsingle block key  Y18.7£ºindicator of single block
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X18.7£ºskip block key  Y18.6:indicator of skip block
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X20.0-optional stop key
COMMENT_END

COMMENT_START
Y21.7-indicator of optional stop
COMMENT_END

BLOCK_INF
sub5


subprogram of rapid move key
BLOCK_INF_END

COMMENT_START
X20.6£ºjog rapid key
   jog rapid is valid in JOG mode
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub6


rigid tap process
BLOCK_INF_END

COMMENT_START
 R6.0£ºmake spindle stop
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Y5.0: spindle V/P switch	

COMMENT_END

COMMENT_START
DT15: time of checking VP(X5.0)after M29 is executed

COMMENT_END

COMMENT_START
DT29: Executive M14, detection VP (X5.1) of the time

COMMENT_END

COMMENT_START
X5.1£ºget spindle zero positon   
Y5.1: TAP singal	

COMMENT_END

COMMENT_START
X5.0: indicator of spindle V/P	

COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub7



BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Y1.3£ºgear 1

COMMENT_END

COMMENT_START
Y1.4£ºgear 2
COMMENT_END

COMMENT_START
Y1.5£ºgear 3
COMMENT_END

COMMENT_START
Y1.6£ºgear 4
COMMENT_END

BLOCK_INF
sub8


adjust feed rate in AUTO¡¢MDI¡¢DNC¡¢EDIT mode
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub9


adjust feed rate in REF¡¢MPG¡¢STEP¡¢JOG mode
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub10


X direction define
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub11


Y direction define
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub12


Z direction define
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub13


4th axis direction define
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub14


5th axis direction define.
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
X25.6:5th direction key   R19.1£º5th:-

COMMENT_END

COMMENT_START
X20.1£º5th direction key£¬R19.2£º5th:+
COMMENT_END

BLOCK_INF
sub15


spindle brake subprogram
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Y0.7:output signal of spindle brake
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub16


output of alternative lubrication
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
Y0.1£ºoutput of lubrication
COMMENT_END

BLOCK_INF
sub17


output of schedular lubrication
BLOCK_INF_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub18


output of auto lubrication
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub19


choose mode
BLOCK_INF_END

COMMENT_START
X18.1£ºAUTO key
COMMENT_END

COMMENT_START
X18.1£ºAUTO key
COMMENT_END

COMMENT_START
X18.2£ºMDI key
COMMENT_END

COMMENT_START
X18.3£ºREF key
COMMENT_END

COMMENT_START
X18.4£ºMPG/STEP key
COMMENT_END

COMMENT_START
X18.5£ºJOG key
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
auto mode
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub20


move subprogram
BLOCK_INF_END

COMMENT_START
4th REF:-
COMMENT_END

COMMENT_START
4th:REF:+
COMMENT_END

COMMENT_START
4th:+ move
COMMENT_END

COMMENT_START
4th:- move
COMMENT_END

COMMENT_START
Y22.4£ºindicator of 4th ref

COMMENT_END

BLOCK_INF
sub21


ove subprogram
BLOCK_INF_END

COMMENT_START
5th:- move
COMMENT_END

COMMENT_START
5th:+ move
COMMENT_END

COMMENT_START
5th:+ move
COMMENT_END

COMMENT_START
5th:- move
COMMENT_END

BLOCK_INF
sub22


µÚ¶þÖ÷Öá¹¦ÄÜ
BLOCK_INF_END

COMMENT_START
R60.3£ºM63 the second spindle ccw
R60.4£ºM64 the second spindle cw
R60.5£ºM65 the second spindle stop
COMMENT_END

COMMENT_START
the first spindle 
COMMENT_END

COMMENT_START
the second spindle 
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Y3.4: the second spindle ccw	
Y3.3: the second spindle cw	
A0.7: M63¡¢M64 error

COMMENT_END

COMMENT_START
X21.5£ºthe spindle stop

COMMENT_END

COMMENT_START
X21.3£ºccw

COMMENT_END

COMMENT_START
X21.7£ºcw
COMMENT_END

COMMENT_START
X25.5£ºjog
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
ccw
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Y2.0:cw
Y3.3: the second spindle cw	

COMMENT_END

COMMENT_START
Y3.3: the second spindle cw	

COMMENT_END

COMMENT_START
Y3.4: the second spindle ccw	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub23


µÚ¶þÖ÷ÖáÖÆ¶¯´¦Àí
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub24


M41TO44×Ô¶¯»»µ²
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
X1.6: Detection of the first tranche of the spindle in place	
X2.6: Detection of the second tranche of the spindle in place	
X3.3: Detection of the third tranche of the spindle in place	
X3.4: Detection of the fourth tranche of the spindle in place	

COMMENT_END

COMMENT_START
DT31: Spindle speed automatic shift
DT32: Automatic gear shift off the original time

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X1.6: Detection of the first tranche of the spindle in place	
DT33: Automatic transmission in place after the end of time delay
X2.6: Detection of the second tranche of the spindle in place	
X3.3: Detection of the third tranche of the spindle in place	
X3.4: Detection of the fourth tranche of the spindle in place	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Automatic shift detection time
COMMENT_END

BLOCK_INF
sub25


Ö÷Öá×Ô¶¯»»µ²Êä³ö
BLOCK_INF_END

COMMENT_START
gear signal 1

COMMENT_END

COMMENT_START
gear signal 2
COMMENT_END

COMMENT_START
gear signal 3
COMMENT_END

COMMENT_START
gear signal 4
COMMENT_END

COMMENT_START
K12.0: 1/0:Spindle automatic transmission signal to keep / not keep	
Y1.0: Spindle mechanical gear signal 1	
X1.6: Detection of the first tranche of the spindle in place	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub26


M54_M55Ö÷ÖáËÉ½ôµ¶
BLOCK_INF_END

COMMENT_START
R50.4(M54)---release tool              R50.5(M55)---clamping tool
COMMENT_END

COMMENT_START
X1.7: Loosen the spindle position check tool	

COMMENT_END

COMMENT_START
Y0.4: SRV,Spindle CW signal	
X1.5: External Elastic tool spindle input signal	
Y0.3: SFR,Spindle CCW signal	
Y5.3: the first spindle cw	
Y5.2: the first spindle ccw	

COMMENT_END

COMMENT_START
no rotation
COMMENT_END

COMMENT_START
X1.5: External Elastic tool spindle input signal	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Y2.0: the clamping/releasing tool signal	

COMMENT_END

COMMENT_START
X2.0: check the clamping tool	
DT30: Elastic the spindle tool  delay time

COMMENT_END

COMMENT_START
DT30: Elastic the spindle tool  delay time

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
M54¡¢M55 completing signal
COMMENT_END

BLOCK_INF
sub30


BT50Ô²ÅÌÐÍ
BLOCK_INF_END

COMMENT_START
R60.5(M65)---the pocket down         R60.6(M66)---the pocket up

COMMENT_END

COMMENT_START
R61.0(M68)---ATC arm seizing tool      R61.1(M69)---ATC arm exchaging tool   R61.2(M70)---ATC arm back
COMMENT_END

COMMENT_START
X2.1: ATC arm motor overload(discal tool)	

COMMENT_END

COMMENT_START
X2.2: tool motor overload(discal tool/armless tool)	
Y1.6: tool motor cw	
Y1.7: tool motor ccw	

COMMENT_END

COMMENT_START
X0.2: cylinder pressure check	
K11.1: 1/0:Does not detect / detect cylinder pressure is too low	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
K11.2: 1/0:Exchange before testing tool / does not detect the reference point	
X5.2: coin signal	

COMMENT_END

COMMENT_START
X1.2: ATC arm back the origin check(discal tool)	
K11.0: ATC arm is not in place 1:Locked to the signal 0: Not locked to the signal	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
completing signal
R20.0--M65
R20.1--M68
R20.4--M69
R20.5--M70
R20.6--M66

COMMENT_END

BLOCK_INF
sub31


BT50Ô²ÅÌÐÍ_µ¶ÅÌ»ØÁã
BLOCK_INF_END

COMMENT_START
X0.6: Pocket level in place/Cutter back in place	
Y1.6: tool motor cw	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X0.0: tool to zero signal	
D409: The current number of pocket
D408: Target No Pocket

COMMENT_END

BLOCK_INF
sub32


BT50Ô²ÅÌÐÍ_ÊÖ¶¯»»µ¶
BLOCK_INF_END

COMMENT_START
jog exchange tool
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D409: The current number of pocket
D408: Target No Pocket

COMMENT_END

BLOCK_INF
sub33


BT50Ô²ÅÌÐÍ_×Ô¶¯»»µ¶
BLOCK_INF_END

COMMENT_START
R276.0:tool rotation signal

COMMENT_END

COMMENT_START
R211.0£ºT function completing signal 
COMMENT_END

COMMENT_START
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
D408: Target No Pocket
D409: The current number of pocket

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub34


BT50Ô²ÅÌÐÍ_¸üÐÂµ¶Ì×µ¶¾ßºÅ
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
exchange number
D409: The current number of pocket

COMMENT_END

COMMENT_START
D411: The tool of number under the pocket number 1
COMMENT_END

COMMENT_START
D409: The current number of pocket

COMMENT_END

COMMENT_START
D412: The tool of number under the pocket number 2
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D413: The tool of number under the pocket number 3
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D415: The tool of number under the pocket number 5
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D416: The tool of number under the pocket number 6

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D418: The tool of number under the pocket number 8
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D419: The tool of number under the pocket number 9
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D420: The tool of number under the pocket number 10
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D421: The tool of number under the pocket number 11
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D422: The tool of number under the pocket number 12
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D423: The tool of number under the pocket number 13
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D424: The tool of number under the pocket number 14
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D425: The tool of number under the pocket number 15
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D426: The tool of number under the pocket number 16
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D427: The tool of number under the pocket number 17
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D428: The tool of number under the pocket number 18
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 19
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 20
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 21
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 22
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 23
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 24
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 25
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 26
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 27
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 28
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 29
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 30
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 31
D410: The current number of pockets on the spindle

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 32
D410: The current number of pockets on the spindle

COMMENT_END

BLOCK_INF
sub35


BT50Ô²ÅÌÐÍ_È¡T¶ÔÓ¦µÄµ¶Ì×ºÅ
BLOCK_INF_END

COMMENT_START
D411: The tool of number under the pocket number 1

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D412: The tool of number under the pocket number 2

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D413: The tool of number under the pocket number 3

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D414: The tool of number under the pocket number 4

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D415: The tool of number under the pocket number 5

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D416: The tool of number under the pocket number 6

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D417: The tool of number under the pocket number 7

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D418: The tool of number under the pocket number 8

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D419: The tool of number under the pocket number 9

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D420: The tool of number under the pocket number 10

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D421: The tool of number under the pocket number 11

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D422: The tool of number under the pocket number 12

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D423: The tool of number under the pocket number 13

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D424: The tool of number under the pocket number 14

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D425: The tool of number under the pocket number 15

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D426: The tool of number under the pocket number 16

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D427: The tool of number under the pocket number 17

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D428: The tool of number under the pocket number 18

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D429: The tool of number under the pocket number 19

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D430: The tool of number under the pocket number 20

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Ä¿±êµ¶Ì×Îª21ºÅµ¶Ì×
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Ä¿±êµ¶Ì×Îª22ºÅµ¶Ì×
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Ä¿±êµ¶Ì×Îª23ºÅµ¶Ì×
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Ä¿±êµ¶Ì×Îª24ºÅµ¶Ì×
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Ä¿±êµ¶Ì×Îª25ºÅµ¶Ì×
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Ä¿±êµ¶Ì×Îª26ºÅµ¶Ì×
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Ä¿±êµ¶Ì×Îª27ºÅµ¶Ì×
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Ä¿±êµ¶Ì×Îª28ºÅµ¶Ì×
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Ä¿±êµ¶Ì×Îª29ºÅµ¶Ì×
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Ä¿±êµ¶Ì×Îª30ºÅµ¶Ì×
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Ä¿±êµ¶Ì×Îª31ºÅµ¶Ì×
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Ä¿±êµ¶Ì×Îª32ºÅµ¶Ì×
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub36


BT50Ô²ÅÌÐÍ_µ¶ÅÌÑ¡µ¶
BLOCK_INF_END

COMMENT_START
X0.6: Pocket level in place/Cutter back in place	
Y1.6: tool motor cw	
Y1.7: tool motor ccw	

COMMENT_END

COMMENT_START
X0.6: Pocket level in place/Cutter back in place	

COMMENT_END

COMMENT_START
D409: The current number of pocket
D408: Target No Pocket

COMMENT_END

COMMENT_START
Y1.7: tool motor ccw	
Y1.6: tool motor cw	

COMMENT_END

COMMENT_START
Y1.6: tool motor cw	
Y1.7: tool motor ccw	

COMMENT_END

BLOCK_INF
sub37


BT50Ô²ÅÌÐÍ_µ¶ÅÌµ¶¾ß¼ÆÊý
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X0.4: take count of tool	
Y1.6: tool motor cw	

COMMENT_END

COMMENT_START
X0.4: take count of tool	
Y1.7: tool motor ccw	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Y1.6: tool motor cw	
D409: The current number of pocket
Y1.7: tool motor ccw	

COMMENT_END

COMMENT_START
Y1.6: tool motor cw	
D409: The current number of pocket
D408: Target No Pocket
Y1.7: tool motor ccw	
DT28: Tool time for pre-cutter

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
G54.0--exchange tool completing
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub38


BT50Ô²ÅÌÐÍ_M65M66µ¶Ì×¶¯×÷
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
X0.7: Vertical pocket in place/Cutter in place ahead	
X1.2: ATC arm back the origin check(discal tool)	
Y1.6: tool motor cw	
Y1.7: tool motor ccw	
Y1.4: Vertical pocket/Cutter Forward	

COMMENT_END

COMMENT_START
X0.7: Vertical pocket in place/Cutter in place ahead	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
R30.3:the pocket up
COMMENT_END

COMMENT_START
Y1.5: Pocket level/Cutter back	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub39


BT50Ô²ÅÌÐÍ_»»µ¶±Û¶¯×÷
BLOCK_INF_END

COMMENT_START
X1.0: ATC arm stop checking(discal tool)	

COMMENT_END

COMMENT_START
X1.1: ATC arm to seize the tool checks(discal tool)	

COMMENT_END

COMMENT_START
X0.7: Vertical pocket in place/Cutter in place ahead	
X1.7: Loosen the spindle position check tool	
K11.3: 1/0:Exchange of tool, the detection / non-detection tool knife Elastic state	
X1.2: ATC arm back the origin check(discal tool)	
X2.0: check the clamping tool	

COMMENT_END

COMMENT_START
Y2.1: ATC arm  motor output signal	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub40


¶·óÒÊ½µ¶¿â
BLOCK_INF_END

COMMENT_START
R60.0(M60)---tool rotation   R60.1(M61)---tool complete
R60.5(M65)---tool forward         R60.6(M66)---tool back
COMMENT_END

COMMENT_START
Y1.6: tool motor cw	
Y1.7: tool motor ccw	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X2.2: tool motor overload(discal tool/armless tool)	
COMMENT_END

COMMENT_START
X0.2: cylinder pressure check	
K11.1: 1/0:Does not detect / detect cylinder pressure is too low	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
K11.2: 1/0:Exchange before testing tool / does not detect the reference point	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
tool count
COMMENT_END

COMMENT_START
D409: The current number of pocket

COMMENT_END

COMMENT_START
DT26: Armless type ATC M instruction execution time

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub41


¶·óÒÊ½_µ¶ÅÌ»ØÁã
BLOCK_INF_END

COMMENT_START
X0.6: Pocket level in place/Cutter back in place	
Y1.6: tool motor cw	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X0.0: tool to zero signal	
COMMENT_END

BLOCK_INF
sub42


¶·óÒÊ½_ÊÖ¶¯»»µ¶
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D409: The current number of pocket
D408: Target No Pocket

COMMENT_END

BLOCK_INF
sub43


¶·óÒÊ½_×Ô¶¯»»µ¶
BLOCK_INF_END

COMMENT_START
D408: Target No Pocket

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
D408: Target No Pocket
D409: The current number of pocket

COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub44


¶·óÒÊ½_M6566µ¶¿â½øÍË
BLOCK_INF_END

COMMENT_START
X3.4: Detection of the fourth tranche of the spindle in place	
Y1.7: tool motor ccw	
X0.7: Vertical pocket in place/Cutter in place ahead	
Y1.6: tool motor cw	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X0.7: Vertical pocket in place/Cutter in place ahead	

COMMENT_END

COMMENT_START
X3.3: Detection of the third tranche of the spindle in place	
Y1.7: tool motor ccw	
X0.7: Vertical pocket in place/Cutter in place ahead	
Y1.6: tool motor cw	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X0.6: Pocket level in place/Cutter back in place	

COMMENT_END

BLOCK_INF
sub45


¶·óÒÊ½_µ¶ÅÌÐý×ª
BLOCK_INF_END

COMMENT_START
K11.4: 1/0:Exchange before testing tool / does not detect the third reference point	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
tool cw
COMMENT_END

COMMENT_START
tool ccw
COMMENT_END

BLOCK_INF
sub46


¶·óÒÊ½_µ¶ÅÌµ¶¾ß¼ÆÊý
BLOCK_INF_END

COMMENT_START
X0.4: take count of tool	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
X0.4: take count of tool	
Y1.6: tool motor cw	

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
Y1.6: tool motor cw	
D409: The current number of pocket
Y1.7: tool motor ccw	

COMMENT_END

COMMENT_START
DT28: Tool time for pre-cutter

COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
SUB47



BLOCK_INF_END

COMMENT_START
total number of tools is 8 
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
total number of tools is 16
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
total number of tools is 20
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
total number of tools is 24
COMMENT_END

COMMENT_START
COMMENT_END

COMMENT_START
total number of tools is 32
COMMENT_END

COMMENT_START
COMMENT_END

BLOCK_INF
sub50


³¬³Ì´¦Àí
BLOCK_INF_END

COMMENT_START
COMMENT_END

COMMENT_START
X2.7: X- overtravel limit input	
K15.0: 1/0:X\Y\Zaxis overtravel limi low/high level alarm	

COMMENT_END

COMMENT_START
X3.0: X+ overtravel limit input	
COMMENT_END

COMMENT_START
X3.1: Y- overtravel limit input	
COMMENT_END

COMMENT_START
X3.2: Y+ overtravel limit input	
COMMENT_END

COMMENT_START
X3.6: Z- overtravel limit input		

COMMENT_END

COMMENT_START
X3.7: Z+ overtravel limit input	
COMMENT_END

END_NETWORK_COMMENT_ADDSECTION

INITDATA_FLAG_ADDTOLD2
D0408	
D0409	
D0410	
D0411	
D0412	
D0413	
D0414	
D0415	
D0416	
D0417	
D0418	
D0419	
D0420	
D0421	
D0422	
D0423	
D0424	
D0425	
D0426	
D0427	
D0428	
D0429	
D0430	
D0431	
D0432	
D0433	
D0434	
D0435	
D0436	
D0437	
D0438	
D0439	
D0440	
D0441	
D0442	
DT0014	
DT0015	
DT0016	
DT0017	
DT0018	
DT0019	
DT0020	
DT0021	
DT0022	
DT0023	
DT0024	
DT0025	
DT0026	
DT0027	
DT0028	
DT0029	
DT0030	
DT0031	
DT0032	
DT0033	
DT0034	
END_INITDATA_FLAG_ADDTOLD2

